(footprint "ST_WLCSP-49_Die438"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "WLCSP-49, 3.89x3.74mm, 49 Ball, 7x7 Layout, 0.5mm Pitch, http://www.st.com/resource/en/datasheet/stm32f303r8.pdf#page=112")
	(tags "CSP 49 0.5")
	(solder_mask_margin 0.03)
	(solder_paste_margin 0.01)
	(property "Reference" "REF**"
		(at 0 -2.87 0)
		(layer "F.SilkS")
	)
	(property "Value" "ST_WLCSP-49_Die438"
		(at 0 2.87 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -1.5 -1.5)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A2" smd circle
		(at -1 -1.5)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A3" smd circle
		(at -0.5 -1.5)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A4" smd circle
		(at 0 -1.5)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A5" smd circle
		(at 0.5 -1.5)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A6" smd circle
		(at 1 -1.5)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A7" smd circle
		(at 1.5 -1.5)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B1" smd circle
		(at -1.5 -1)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B2" smd circle
		(at -1 -1)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B3" smd circle
		(at -0.5 -1)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B4" smd circle
		(at 0 -1)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B5" smd circle
		(at 0.5 -1)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B6" smd circle
		(at 1 -1)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B7" smd circle
		(at 1.5 -1)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C1" smd circle
		(at -1.5 -0.5)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C2" smd circle
		(at -1 -0.5)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C3" smd circle
		(at -0.5 -0.5)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C4" smd circle
		(at 0 -0.5)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C5" smd circle
		(at 0.5 -0.5)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C6" smd circle
		(at 1 -0.5)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C7" smd circle
		(at 1.5 -0.5)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D1" smd circle
		(at -1.5 0)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D2" smd circle
		(at -1 0)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D3" smd circle
		(at -0.5 0)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D4" smd circle
		(at 0 0)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D5" smd circle
		(at 0.5 0)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D6" smd circle
		(at 1 0)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D7" smd circle
		(at 1.5 0)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E1" smd circle
		(at -1.5 0.5)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E2" smd circle
		(at -1 0.5)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E3" smd circle
		(at -0.5 0.5)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E4" smd circle
		(at 0 0.5)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E5" smd circle
		(at 0.5 0.5)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E6" smd circle
		(at 1 0.5)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E7" smd circle
		(at 1.5 0.5)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F1" smd circle
		(at -1.5 1)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F2" smd circle
		(at -1 1)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F3" smd circle
		(at -0.5 1)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F4" smd circle
		(at 0 1)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F5" smd circle
		(at 0.5 1)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F6" smd circle
		(at 1 1)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F7" smd circle
		(at 1.5 1)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G1" smd circle
		(at -1.5 1.5)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G2" smd circle
		(at -1 1.5)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G3" smd circle
		(at -0.5 1.5)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G4" smd circle
		(at 0 1.5)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G5" smd circle
		(at 0.5 1.5)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G6" smd circle
		(at 1 1.5)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G7" smd circle
		(at 1.5 1.5)
		(size 0.29 0.29)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_CSP.3dshapes/ST_WLCSP-49_Die438.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
