(footprint "ST_WLCSP-72_Die415"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "WLCSP-72, 4.4084x3.7594mm, 72 Ball, 9x9 Layout, 0.4mm Pitch, http://www.st.com/resource/en/datasheet/stm32l476me.pdf#page=255")
	(tags "CSP 72 0.4")
	(solder_mask_margin 0.0325)
	(solder_paste_margin 0.0125)
	(property "Reference" "REF**"
		(at 0 -2.8797 0)
		(layer "F.SilkS")
	)
	(property "Value" "ST_WLCSP-72_Die415"
		(at 0 2.8797 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -1.6 -1.6)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A2" smd circle
		(at -1.2 -1.6)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A3" smd circle
		(at -0.8 -1.6)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A4" smd circle
		(at -0.4 -1.6)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A5" smd circle
		(at 0 -1.6)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A6" smd circle
		(at 0.4 -1.6)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A7" smd circle
		(at 0.8 -1.6)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A8" smd circle
		(at 1.2 -1.6)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A9" smd circle
		(at 1.6 -1.6)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B1" smd circle
		(at -1.6 -1.2)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B2" smd circle
		(at -1.2 -1.2)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B3" smd circle
		(at -0.8 -1.2)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B4" smd circle
		(at -0.4 -1.2)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B5" smd circle
		(at 0 -1.2)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B6" smd circle
		(at 0.4 -1.2)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B7" smd circle
		(at 0.8 -1.2)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B8" smd circle
		(at 1.2 -1.2)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B9" smd circle
		(at 1.6 -1.2)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C1" smd circle
		(at -1.6 -0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C2" smd circle
		(at -1.2 -0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C3" smd circle
		(at -0.8 -0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C4" smd circle
		(at -0.4 -0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C5" smd circle
		(at 0 -0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C6" smd circle
		(at 0.4 -0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C7" smd circle
		(at 0.8 -0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C8" smd circle
		(at 1.2 -0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C9" smd circle
		(at 1.6 -0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D1" smd circle
		(at -1.6 -0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D2" smd circle
		(at -1.2 -0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D3" smd circle
		(at -0.8 -0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D7" smd circle
		(at 0.8 -0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D8" smd circle
		(at 1.2 -0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D9" smd circle
		(at 1.6 -0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E1" smd circle
		(at -1.6 0)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E2" smd circle
		(at -1.2 0)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E3" smd circle
		(at -0.8 0)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E7" smd circle
		(at 0.8 0)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E8" smd circle
		(at 1.2 0)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E9" smd circle
		(at 1.6 0)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F1" smd circle
		(at -1.6 0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F2" smd circle
		(at -1.2 0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F3" smd circle
		(at -0.8 0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F7" smd circle
		(at 0.8 0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F8" smd circle
		(at 1.2 0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F9" smd circle
		(at 1.6 0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G1" smd circle
		(at -1.6 0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G2" smd circle
		(at -1.2 0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G3" smd circle
		(at -0.8 0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G4" smd circle
		(at -0.4 0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G5" smd circle
		(at 0 0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G6" smd circle
		(at 0.4 0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G7" smd circle
		(at 0.8 0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G8" smd circle
		(at 1.2 0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G9" smd circle
		(at 1.6 0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H1" smd circle
		(at -1.6 1.2)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H2" smd circle
		(at -1.2 1.2)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H3" smd circle
		(at -0.8 1.2)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H4" smd circle
		(at -0.4 1.2)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H5" smd circle
		(at 0 1.2)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H6" smd circle
		(at 0.4 1.2)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H7" smd circle
		(at 0.8 1.2)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H8" smd circle
		(at 1.2 1.2)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H9" smd circle
		(at 1.6 1.2)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J1" smd circle
		(at -1.6 1.6)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J2" smd circle
		(at -1.2 1.6)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J3" smd circle
		(at -0.8 1.6)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J4" smd circle
		(at -0.4 1.6)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J5" smd circle
		(at 0 1.6)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J6" smd circle
		(at 0.4 1.6)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J7" smd circle
		(at 0.8 1.6)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J8" smd circle
		(at 1.2 1.6)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J9" smd circle
		(at 1.6 1.6)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_CSP.3dshapes/ST_WLCSP-72_Die415.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
