(footprint "WLCSP-16_2.225x2.17mm_Layout4x4_P0.5mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "WLCSP-16 2.225x2.17mm, 2.225x2.17mm, 16 Ball, 4x4 Layout, 0.5mm Pitch, https://ww1.microchip.com/downloads/en/DeviceDoc/16B_WLCSP_CS_C04-06036c.pdf")
	(tags "CSP 16 0.5")
	(property "Reference" "REF**"
		(at 0 -2.085 0)
		(layer "F.SilkS")
	)
	(property "Value" "WLCSP-16_2.225x2.17mm_Layout4x4_P0.5mm"
		(at 0 2.085 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -0.75 -0.75)
		(size 0.327 0.327)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A2" smd circle
		(at -0.25 -0.75)
		(size 0.327 0.327)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A3" smd circle
		(at 0.25 -0.75)
		(size 0.327 0.327)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A4" smd circle
		(at 0.75 -0.75)
		(size 0.327 0.327)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B1" smd circle
		(at -0.75 -0.25)
		(size 0.327 0.327)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B2" smd circle
		(at -0.25 -0.25)
		(size 0.327 0.327)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B3" smd circle
		(at 0.25 -0.25)
		(size 0.327 0.327)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B4" smd circle
		(at 0.75 -0.25)
		(size 0.327 0.327)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C1" smd circle
		(at -0.75 0.25)
		(size 0.327 0.327)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C2" smd circle
		(at -0.25 0.25)
		(size 0.327 0.327)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C3" smd circle
		(at 0.25 0.25)
		(size 0.327 0.327)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C4" smd circle
		(at 0.75 0.25)
		(size 0.327 0.327)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D1" smd circle
		(at -0.75 0.75)
		(size 0.327 0.327)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D2" smd circle
		(at -0.25 0.75)
		(size 0.327 0.327)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D3" smd circle
		(at 0.25 0.75)
		(size 0.327 0.327)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D4" smd circle
		(at 0.75 0.75)
		(size 0.327 0.327)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_CSP.3dshapes/WLCSP-16_2.225x2.17mm_Layout4x4_P0.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
