(footprint "WLCSP-20_1.934x2.434mm_Layout4x5_P0.4mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "WLCSP-20, 4x5 raster, 1.934x2.434mm package, pitch 0.4mm; see section 36.2.3 of http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-42363-SAM-D11_Datasheet.pdf")
	(tags "BGA 20 0.4")
	(property "Reference" "REF**"
		(at 0 -2.7 0)
		(layer "F.SilkS")
	)
	(property "Value" "WLCSP-20_1.934x2.434mm_Layout4x5_P0.4mm"
		(at 0 2.217 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -0.6 -0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio 0.055556)
	)
	(pad "A2" smd circle
		(at -0.2 -0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio 0.055556)
	)
	(pad "A3" smd circle
		(at 0.2 -0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio 0.055556)
	)
	(pad "A4" smd circle
		(at 0.6 -0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio 0.055556)
	)
	(pad "B1" smd circle
		(at -0.6 -0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio 0.055556)
	)
	(pad "B2" smd circle
		(at -0.2 -0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio 0.055556)
	)
	(pad "B3" smd circle
		(at 0.2 -0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio 0.055556)
	)
	(pad "B4" smd circle
		(at 0.6 -0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio 0.055556)
	)
	(pad "C1" smd circle
		(at -0.6 0)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio 0.055556)
	)
	(pad "C2" smd circle
		(at -0.2 0)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio 0.055556)
	)
	(pad "C3" smd circle
		(at 0.2 0)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio 0.055556)
	)
	(pad "C4" smd circle
		(at 0.6 0)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio 0.055556)
	)
	(pad "D1" smd circle
		(at -0.6 0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio 0.055556)
	)
	(pad "D2" smd circle
		(at -0.2 0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio 0.055556)
	)
	(pad "D3" smd circle
		(at 0.2 0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio 0.055556)
	)
	(pad "D4" smd circle
		(at 0.6 0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio 0.055556)
	)
	(pad "E1" smd circle
		(at -0.6 0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio 0.055556)
	)
	(pad "E2" smd circle
		(at -0.2 0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio 0.055556)
	)
	(pad "E3" smd circle
		(at 0.2 0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio 0.055556)
	)
	(pad "E4" smd circle
		(at 0.6 0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio 0.055556)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_CSP.3dshapes/WLCSP-20_1.934x2.434mm_Layout4x5_P0.4mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
