(footprint "WLCSP-36_2.374x2.459mm_Layout6x6_P0.35mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "WLCSP-36, https://www.nxp.com/docs/en/package-information/98ASA00604D.pdf")
	(tags "WLCSP-36")
	(property "Reference" "REF**"
		(at 0 -3.34 0)
		(layer "F.SilkS")
	)
	(property "Value" "WLCSP-36_2.374x2.459mm_Layout6x6_P0.35mm"
		(at 0 3.43 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -0.875 -0.875)
		(size 0.274 0.274)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd circle
		(at -0.525 -0.875)
		(size 0.274 0.274)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd circle
		(at -0.175 -0.875)
		(size 0.274 0.274)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A4" smd circle
		(at 0.175 -0.875)
		(size 0.274 0.274)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A5" smd circle
		(at 0.525 -0.875)
		(size 0.274 0.274)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A6" smd circle
		(at 0.875 -0.875)
		(size 0.274 0.274)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd circle
		(at -0.875 -0.525)
		(size 0.274 0.274)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B2" smd circle
		(at -0.525 -0.525)
		(size 0.274 0.274)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B3" smd circle
		(at -0.175 -0.525)
		(size 0.274 0.274)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B4" smd circle
		(at 0.175 -0.525)
		(size 0.274 0.274)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B5" smd circle
		(at 0.525 -0.525)
		(size 0.274 0.274)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B6" smd circle
		(at 0.875 -0.525)
		(size 0.274 0.274)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C1" smd circle
		(at -0.875 -0.175)
		(size 0.274 0.274)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C2" smd circle
		(at -0.525 -0.175)
		(size 0.274 0.274)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C3" smd circle
		(at -0.175 -0.175)
		(size 0.274 0.274)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C4" smd circle
		(at 0.175 -0.175)
		(size 0.274 0.274)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C5" smd circle
		(at 0.525 -0.175)
		(size 0.274 0.274)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C6" smd circle
		(at 0.875 -0.175)
		(size 0.274 0.274)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D1" smd circle
		(at -0.875 0.175)
		(size 0.274 0.274)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D2" smd circle
		(at -0.525 0.175)
		(size 0.274 0.274)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D3" smd circle
		(at -0.175 0.175)
		(size 0.274 0.274)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D4" smd circle
		(at 0.175 0.175)
		(size 0.274 0.274)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D5" smd circle
		(at 0.525 0.175)
		(size 0.274 0.274)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D6" smd circle
		(at 0.875 0.175)
		(size 0.274 0.274)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E1" smd circle
		(at -0.875 0.525)
		(size 0.274 0.274)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E2" smd circle
		(at -0.525 0.525)
		(size 0.274 0.274)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E3" smd circle
		(at -0.175 0.525)
		(size 0.274 0.274)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E4" smd circle
		(at 0.175 0.525)
		(size 0.274 0.274)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E5" smd circle
		(at 0.525 0.525)
		(size 0.274 0.274)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E6" smd circle
		(at 0.875 0.525)
		(size 0.274 0.274)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F1" smd circle
		(at -0.875 0.875)
		(size 0.274 0.274)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F2" smd circle
		(at -0.525 0.875)
		(size 0.274 0.274)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F3" smd circle
		(at -0.175 0.875)
		(size 0.274 0.274)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F4" smd circle
		(at 0.175 0.875)
		(size 0.274 0.274)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F5" smd circle
		(at 0.525 0.875)
		(size 0.274 0.274)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F6" smd circle
		(at 0.875 0.875)
		(size 0.274 0.274)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_CSP.3dshapes/WLCSP-36_2.374x2.459mm_Layout6x6_P0.35mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
