(footprint "WLCSP-4_0.64x0.64mm_Layout2x2_P0.35mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "WLCSP-4, 0.64x0.64mm, 4 Ball, 2x2 Layout, 0.35mm Pitch, https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf#page=23")
	(tags "CSP 4 0.35")
	(property "Reference" "REF**"
		(at 0 -1.32 0)
		(layer "F.SilkS")
	)
	(property "Value" "WLCSP-4_0.64x0.64mm_Layout2x2_P0.35mm"
		(at 0 1.32 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -0.175 -0.175)
		(size 0.21 0.21)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A2" smd circle
		(at 0.175 -0.175)
		(size 0.21 0.21)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B1" smd circle
		(at -0.175 0.175)
		(size 0.21 0.21)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B2" smd circle
		(at 0.175 0.175)
		(size 0.21 0.21)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_CSP.3dshapes/WLCSP-4_0.64x0.64mm_Layout2x2_P0.35mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
