(footprint "WLCSP-8_1.58x1.63x0.35mm_Layout3x5_P0.35x0.4mm_Ball0.25mm_Pad0.25mm_NSMD"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "WLCSP/XFBGA 8-pin package, staggered pins, http://www.adestotech.com/wp-content/uploads/DS-AT25DF041B_040.pdf")
	(tags "WLCSP WLCSP-8 XFBGA XFBGA-8  CSP BGA Chip-Scale Glass-Top")
	(property "Reference" "REF**"
		(at 0 -2.31 0)
		(layer "F.SilkS")
	)
	(property "Value" "WLCSP-8_1.58x1.63x0.35mm_Layout3x5_P0.35x0.4mm_Ball0.25mm_Pad0.25mm_NSMD"
		(at 0 2.76 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -0.35 -0.4)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "A3" smd circle
		(at 0.35 -0.4)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "B2" smd circle
		(at 0 -0.2)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "C1" smd circle
		(at -0.35 0)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "C3" smd circle
		(at 0.35 0)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "D2" smd circle
		(at 0 0.2)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "E1" smd circle
		(at -0.35 0.4)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "E3" smd circle
		(at 0.35 0.4)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_CSP.3dshapes/WLCSP-8_1.58x1.63x0.35mm_Layout3x5_P0.35x0.4mm_Ball0.25mm_Pad0.25mm_NSMD.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
