(footprint "pSemi_CSP-16_1.64x2.04mm_P0.4mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "pSemi CSP-16 1.64x2.04x0.285mm (http://www.psemi.com/pdf/datasheets/pe29101ds.pdf, http://www.psemi.com/pdf/app_notes/an77.pdf)")
	(tags "psemi csp 16")
	(property "Reference" "REF**"
		(at 0 -2.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "pSemi_CSP-16_1.64x2.04mm_P0.4mm"
		(at 0 2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "1" smd circle
		(at -0.6 -0.8)
		(size 0.09 0.09)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd circle
		(at -0.6 -0.4)
		(size 0.09 0.09)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd circle
		(at -0.6 0)
		(size 0.09 0.09)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd circle
		(at -0.6 0.4)
		(size 0.09 0.09)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd circle
		(at -0.6 0.8)
		(size 0.09 0.09)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd circle
		(at -0.2 -0.8)
		(size 0.09 0.09)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd circle
		(at -0.2 0.4)
		(size 0.09 0.09)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd circle
		(at -0.2 0.8)
		(size 0.09 0.09)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd circle
		(at 0.2 -0.8)
		(size 0.09 0.09)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd circle
		(at 0.2 0.4)
		(size 0.09 0.09)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd circle
		(at 0.2 0.8)
		(size 0.09 0.09)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd circle
		(at 0.6 -0.8)
		(size 0.09 0.09)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd circle
		(at 0.6 -0.4)
		(size 0.09 0.09)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd circle
		(at 0.6 0)
		(size 0.09 0.09)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd circle
		(at 0.6 0.4)
		(size 0.09 0.09)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd circle
		(at 0.6 0.8)
		(size 0.09 0.09)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_CSP.3dshapes/pSemi_CSP-16_1.64x2.04mm_P0.4mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
