(footprint "AMS_QFN-4-1EP_2x2mm_P0.95mm_EP0.7x1.6mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "UFD Package, 4-Lead Plastic QFN (2mm x 2mm), http://ams.com/eng/content/download/950231/2267959/483138")
	(tags "QFN 0.95")
	(property "Reference" "REF**"
		(at 0 -2 0)
		(layer "F.SilkS")
	)
	(property "Value" "AMS_QFN-4-1EP_2x2mm_P0.95mm_EP0.7x1.6mm"
		(at 0 2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at 0 0)
		(size 0.35 0.8)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -0.95 -0.475)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.05)
	)
	(pad "2" smd rect
		(at -0.95 0.475)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.05)
	)
	(pad "3" smd rect
		(at 0.95 0.475)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.05)
	)
	(pad "4" smd rect
		(at 0.95 -0.475)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.05)
	)
	(pad "5" smd rect
		(at 0 0)
		(size 0.7 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/AMS_QFN-4-1EP_2x2mm_P0.95mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
