(footprint "AO_DFN-8-1EP_5.55x5.2mm_P1.27mm_EP4.12x4.6mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "DD Package; 8-Lead Plastic DFN (5.55mm x 5.2mm), Pin 5-8 connected to EP (http://www.aosmd.com/res/packaging_information/DFN5x6_8L_EP1_P.pdf)")
	(tags "dfn ")
	(property "Reference" "REF**"
		(at 0 -3.68 0)
		(layer "F.SilkS")
	)
	(property "Value" "AO_DFN-8-1EP_5.55x5.2mm_P1.27mm_EP4.12x4.6mm"
		(at 0 3.73 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -1 -1.65 270)
		(size 0.9 0.78)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1 -0.55 270)
		(size 0.9 0.78)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1 0.55 270)
		(size 0.9 0.78)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1 1.65 270)
		(size 0.9 0.78)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.02 -1.65 270)
		(size 0.9 0.78)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.02 -0.55 270)
		(size 0.9 0.78)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.02 0.55 270)
		(size 0.9 0.78)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.02 1.65 270)
		(size 0.9 0.78)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.96 -1.65 270)
		(size 0.9 0.78)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.96 -0.55 270)
		(size 0.9 0.78)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.96 0.55 270)
		(size 0.9 0.78)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.96 1.65 270)
		(size 0.9 0.78)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.94 -1.65 270)
		(size 0.9 0.78)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.94 -0.55 270)
		(size 0.9 0.78)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.94 0.55 270)
		(size 0.9 0.78)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.94 1.65 270)
		(size 0.9 0.78)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -2.75 -1.905 270)
		(size 0.5 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -2.75 -0.635 270)
		(size 0.5 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -2.75 0.635 270)
		(size 0.5 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -2.75 1.905 270)
		(size 0.5 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 0.465 0 270)
		(size 4.6 4.12)
		(layers "F.Cu" "F.Mask")
	)
	(pad "5" smd rect
		(at 2.8 -1.905 270)
		(size 0.5 0.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 2.8 -0.635 270)
		(size 0.5 0.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 2.8 0.635 270)
		(size 0.5 0.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 2.8 1.905 270)
		(size 0.5 0.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/AO_DFN-8-1EP_5.55x5.2mm_P1.27mm_EP4.12x4.6mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
