(footprint "ArtInChip_QFN-88-1EP_10x10mm_P0.4mm_EP6.74x6.74mm_ThermalVias"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "ArtInChip  QFN, 88 Pin (https://artinchip.com/upload/files/product/20240112/17050529177725663.pdf/#page=43), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "ArtInChip QFN NoLead")
	(property "Reference" "REF**"
		(at 0 -6.03 0)
		(layer "F.SilkS")
	)
	(property "Value" "ArtInChip_QFN-88-1EP_10x10mm_P0.4mm_EP6.74x6.74mm_ThermalVias"
		(at 0 6.03 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -2.08 -2.08)
		(size 1.740261 1.740261)
		(layers "F.Paste")
		(roundrect_rratio 0.143657)
	)
	(pad "" smd roundrect
		(at -2.08 0)
		(size 1.740261 1.740261)
		(layers "F.Paste")
		(roundrect_rratio 0.143657)
	)
	(pad "" smd roundrect
		(at -2.08 2.08)
		(size 1.740261 1.740261)
		(layers "F.Paste")
		(roundrect_rratio 0.143657)
	)
	(pad "" smd roundrect
		(at 0 -2.08)
		(size 1.740261 1.740261)
		(layers "F.Paste")
		(roundrect_rratio 0.143657)
	)
	(pad "" smd roundrect
		(at 0 0)
		(size 1.740261 1.740261)
		(layers "F.Paste")
		(roundrect_rratio 0.143657)
	)
	(pad "" smd roundrect
		(at 0 2.08)
		(size 1.740261 1.740261)
		(layers "F.Paste")
		(roundrect_rratio 0.143657)
	)
	(pad "" smd roundrect
		(at 2.08 -2.08)
		(size 1.740261 1.740261)
		(layers "F.Paste")
		(roundrect_rratio 0.143657)
	)
	(pad "" smd roundrect
		(at 2.08 0)
		(size 1.740261 1.740261)
		(layers "F.Paste")
		(roundrect_rratio 0.143657)
	)
	(pad "" smd roundrect
		(at 2.08 2.08)
		(size 1.740261 1.740261)
		(layers "F.Paste")
		(roundrect_rratio 0.143657)
	)
	(pad "1" smd roundrect
		(at -4.8 -4.2)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -4.8 -3.8)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -4.8 -3.4)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -4.8 -3)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -4.8 -2.6)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -4.8 -2.2)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -4.8 -1.8)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -4.8 -1.4)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -4.8 -1)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -4.8 -0.6)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at -4.8 -0.2)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at -4.8 0.2)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at -4.8 0.6)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at -4.8 1)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at -4.8 1.4)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at -4.8 1.8)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at -4.8 2.2)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at -4.8 2.6)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at -4.8 3)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at -4.8 3.4)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at -4.8 3.8)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at -4.8 4.2)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at -4.2 4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at -3.8 4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd roundrect
		(at -3.4 4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "26" smd roundrect
		(at -3 4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "27" smd roundrect
		(at -2.6 4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd roundrect
		(at -2.2 4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "29" smd roundrect
		(at -1.8 4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "30" smd roundrect
		(at -1.4 4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "31" smd roundrect
		(at -1 4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "32" smd roundrect
		(at -0.6 4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "33" smd roundrect
		(at -0.2 4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "34" smd roundrect
		(at 0.2 4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "35" smd roundrect
		(at 0.6 4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "36" smd roundrect
		(at 1 4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "37" smd roundrect
		(at 1.4 4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "38" smd roundrect
		(at 1.8 4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "39" smd roundrect
		(at 2.2 4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "40" smd roundrect
		(at 2.6 4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "41" smd roundrect
		(at 3 4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "42" smd roundrect
		(at 3.4 4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "43" smd roundrect
		(at 3.8 4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "44" smd roundrect
		(at 4.2 4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "45" smd roundrect
		(at 4.8 4.2)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "46" smd roundrect
		(at 4.8 3.8)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "47" smd roundrect
		(at 4.8 3.4)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "48" smd roundrect
		(at 4.8 3)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "49" smd roundrect
		(at 4.8 2.6)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "50" smd roundrect
		(at 4.8 2.2)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "51" smd roundrect
		(at 4.8 1.8)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "52" smd roundrect
		(at 4.8 1.4)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "53" smd roundrect
		(at 4.8 1)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "54" smd roundrect
		(at 4.8 0.6)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "55" smd roundrect
		(at 4.8 0.2)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "56" smd roundrect
		(at 4.8 -0.2)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "57" smd roundrect
		(at 4.8 -0.6)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "58" smd roundrect
		(at 4.8 -1)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "59" smd roundrect
		(at 4.8 -1.4)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "60" smd roundrect
		(at 4.8 -1.8)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "61" smd roundrect
		(at 4.8 -2.2)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "62" smd roundrect
		(at 4.8 -2.6)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "63" smd roundrect
		(at 4.8 -3)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "64" smd roundrect
		(at 4.8 -3.4)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "65" smd roundrect
		(at 4.8 -3.8)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "66" smd roundrect
		(at 4.8 -4.2)
		(size 0.55 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "67" smd roundrect
		(at 4.2 -4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "68" smd roundrect
		(at 3.8 -4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "69" smd roundrect
		(at 3.4 -4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "70" smd roundrect
		(at 3 -4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "71" smd roundrect
		(at 2.6 -4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "72" smd roundrect
		(at 2.2 -4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "73" smd roundrect
		(at 1.8 -4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "74" smd roundrect
		(at 1.4 -4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "75" smd roundrect
		(at 1 -4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "76" smd roundrect
		(at 0.6 -4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "77" smd roundrect
		(at 0.2 -4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "78" smd roundrect
		(at -0.2 -4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "79" smd roundrect
		(at -0.6 -4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "80" smd roundrect
		(at -1 -4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "81" smd roundrect
		(at -1.4 -4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "82" smd roundrect
		(at -1.8 -4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "83" smd roundrect
		(at -2.2 -4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "84" smd roundrect
		(at -2.6 -4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "85" smd roundrect
		(at -3 -4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "86" smd roundrect
		(at -3.4 -4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "87" smd roundrect
		(at -3.8 -4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "88" smd roundrect
		(at -4.2 -4.8)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "89" thru_hole circle
		(at -3.12 -3.12)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "89" thru_hole circle
		(at -3.12 -1.04)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "89" thru_hole circle
		(at -3.12 1.04)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "89" thru_hole circle
		(at -3.12 3.12)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "89" thru_hole circle
		(at -1.04 -3.12)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "89" thru_hole circle
		(at -1.04 -1.04)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "89" thru_hole circle
		(at -1.04 1.04)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "89" thru_hole circle
		(at -1.04 3.12)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "89" smd rect
		(at 0 0)
		(size 6.74 6.74)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(pad "89" smd rect
		(at 0 0)
		(size 6.74 6.74)
		(property pad_prop_heatsink)
		(layers "B.Cu")
		(zone_connect 2)
	)
	(pad "89" thru_hole circle
		(at 1.04 -3.12)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "89" thru_hole circle
		(at 1.04 -1.04)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "89" thru_hole circle
		(at 1.04 1.04)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "89" thru_hole circle
		(at 1.04 3.12)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "89" thru_hole circle
		(at 3.12 -3.12)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "89" thru_hole circle
		(at 3.12 -1.04)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "89" thru_hole circle
		(at 3.12 1.04)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "89" thru_hole circle
		(at 3.12 3.12)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/ArtInChip_QFN-88-1EP_10x10mm_P0.4mm_EP6.74x6.74mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
