(footprint "DFN-12-1EP_4x4mm_P0.65mm_EP2.64x3.54mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "DFN12, 4x4, 0.65P; CASE 506CE (see ON Semiconductor 506CE.PDF)")
	(tags "DFN 0.65")
	(property "Reference" "REF**"
		(at 0 -3.075 0)
		(layer "F.SilkS")
	)
	(property "Value" "DFN-12-1EP_4x4mm_P0.65mm_EP2.64x3.54mm"
		(at 0 3.075 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -0.66 -1.3275)
		(size 1.1 0.7)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.66 -0.4425)
		(size 1.1 0.7)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.66 0.4425)
		(size 1.1 0.7)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.66 1.3275)
		(size 1.1 0.7)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.66 -1.3275)
		(size 1.1 0.7)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.66 -0.4425)
		(size 1.1 0.7)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.66 0.4425)
		(size 1.1 0.7)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.66 1.3275)
		(size 1.1 0.7)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -1.835 -1.625)
		(size 0.63 0.36)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.835 -0.975)
		(size 0.63 0.36)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.835 -0.325)
		(size 0.63 0.36)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.835 0.325)
		(size 0.63 0.36)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -1.835 0.975)
		(size 0.63 0.36)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -1.835 1.625)
		(size 0.63 0.36)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 1.835 1.625)
		(size 0.63 0.36)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 1.835 0.975)
		(size 0.63 0.36)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 1.835 0.325)
		(size 0.63 0.36)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 1.835 -0.325)
		(size 0.63 0.36)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 1.835 -0.975)
		(size 0.63 0.36)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 1.835 -1.625)
		(size 0.63 0.36)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 0 0)
		(size 2.64 3.54)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/DFN-12-1EP_4x4mm_P0.65mm_EP2.64x3.54mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
