(footprint "DFN-14-1EP_3x3mm_P0.4mm_EP1.78x2.35mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "DD Package; 14-Lead Plastic DFN (3mm x 3mm) (http://pdfserv.maximintegrated.com/land_patterns/90-0063.PDF)")
	(tags "DFN 0.40")
	(property "Reference" "REF**"
		(at 0 -2.55 0)
		(layer "F.SilkS")
	)
	(property "Value" "DFN-14-1EP_3x3mm_P0.4mm_EP1.78x2.35mm"
		(at 0 2.55 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -0.445 -0.5875)
		(size 0.7 0.97)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.445 0.5875)
		(size 0.7 0.97)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.45 -0.5875)
		(size 0.7 0.97)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.45 0.5875)
		(size 0.7 0.97)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -1.475 -1.2)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.475 -0.8)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.475 -0.4)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.475 0)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -1.475 0.4)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -1.475 0.8)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -1.475 1.2)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 1.475 1.2)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 1.475 0.8)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 1.475 0.4)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 1.475 0)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 1.475 -0.4)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 1.475 -0.8)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 1.475 -1.2)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 0 0)
		(size 1.78 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/DFN-14-1EP_3x3mm_P0.4mm_EP1.78x2.35mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
