(footprint "DFN-14-1EP_3x4.5mm_P0.65mm_EP1.65x4.25mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "14-lead very thin plastic quad flat, 3.0x4.5mm size, 0.65mm pitch (http://ww1.microchip.com/downloads/en/DeviceDoc/14L_VDFN_4_5x3_0mm_JHA_C041198A.pdf)")
	(tags "VDFN DFN 0.65mm")
	(property "Reference" "REF**"
		(at 0 -3.45 0)
		(layer "F.SilkS")
	)
	(property "Value" "DFN-14-1EP_3x4.5mm_P0.65mm_EP1.65x4.25mm"
		(at 0 3.65 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -0.4125 -1.59375)
		(size 0.66 0.85)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.4125 -0.53125)
		(size 0.66 0.85)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.4125 0.53125)
		(size 0.66 0.85)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.4125 1.59375)
		(size 0.66 0.85)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.4125 -1.59375)
		(size 0.66 0.85)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.4125 -0.53125)
		(size 0.66 0.85)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.4125 0.53125)
		(size 0.66 0.85)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.4125 1.59375)
		(size 0.66 0.85)
		(layers "F.Paste")
	)
	(pad "1" smd oval
		(at -1.5 -1.95)
		(size 0.85 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd oval
		(at -1.5 -1.3)
		(size 0.85 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd oval
		(at -1.5 -0.65)
		(size 0.85 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd oval
		(at -1.5 0)
		(size 0.85 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd oval
		(at -1.5 0.65)
		(size 0.85 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd oval
		(at -1.5 1.3)
		(size 0.85 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd oval
		(at -1.5 1.95)
		(size 0.85 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd oval
		(at 1.5 1.95)
		(size 0.85 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd oval
		(at 1.5 1.3)
		(size 0.85 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd oval
		(at 1.5 0.65)
		(size 0.85 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd oval
		(at 1.5 0)
		(size 0.85 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd oval
		(at 1.5 -0.65)
		(size 0.85 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd oval
		(at 1.5 -1.3)
		(size 0.85 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd oval
		(at 1.5 -1.95)
		(size 0.85 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 0 0)
		(size 1.65 4.25)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/DFN-14-1EP_3x4.5mm_P0.65mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
