(footprint "DFN-14_1.35x3.5mm_P0.5mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "DFN, 14 Pin (https://m.littelfuse.com/media?resourcetype=datasheets&itemid=9fbe09c9-efee-4022-a889-ca0005cd9b07&filename=littelfuse-tvs-diode-array-sp3012-datasheet#page=5), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "DFN NoLead")
	(property "Reference" "REF**"
		(at 0 -2.7 0)
		(layer "F.SilkS")
	)
	(property "Value" "DFN-14_1.35x3.5mm_P0.5mm"
		(at 0 2.7 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.625 -1.5)
		(size 0.85 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -0.625 -1)
		(size 0.85 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -0.625 -0.5)
		(size 0.85 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -0.625 0)
		(size 0.85 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -0.625 0.5)
		(size 0.85 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -0.625 1)
		(size 0.85 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -0.625 1.5)
		(size 0.85 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 0.625 1.5)
		(size 0.85 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at 0.625 1)
		(size 0.85 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at 0.625 0.5)
		(size 0.85 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at 0.625 0)
		(size 0.85 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at 0.625 -0.5)
		(size 0.85 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 0.625 -1)
		(size 0.85 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at 0.625 -1.5)
		(size 0.85 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/DFN-14_1.35x3.5mm_P0.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
