(footprint "DFN-18-1EP_3x5mm_P0.5mm_EP1.66x4.4mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "DHC Package; 18-Lead Plastic DFN (5mm x 3mm) (see Linear Technology 05081955_0_DHC18.pdf)")
	(tags "DFN 0.5")
	(property "Reference" "REF**"
		(at 0 -3.55 0)
		(layer "F.SilkS")
	)
	(property "Value" "DFN-18-1EP_3x5mm_P0.5mm_EP1.66x4.4mm"
		(at 0 3.55 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -0.415 -1.76)
		(size 0.67 0.71)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.415 -0.88)
		(size 0.67 0.71)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.415 0)
		(size 0.67 0.71)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.415 0.88)
		(size 0.67 0.71)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.415 1.76)
		(size 0.67 0.71)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.415 -1.76)
		(size 0.67 0.71)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.415 -0.88)
		(size 0.67 0.71)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.415 0)
		(size 0.67 0.71)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.415 0.88)
		(size 0.67 0.71)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.415 1.76)
		(size 0.67 0.71)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -1.425 -2)
		(size 0.65 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.425 -1.5)
		(size 0.65 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.425 -1)
		(size 0.65 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.425 -0.5)
		(size 0.65 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -1.425 0)
		(size 0.65 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -1.425 0.5)
		(size 0.65 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -1.425 1)
		(size 0.65 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -1.425 1.5)
		(size 0.65 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -1.425 2)
		(size 0.65 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 1.425 2)
		(size 0.65 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 1.425 1.5)
		(size 0.65 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 1.425 1)
		(size 0.65 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 1.425 0.5)
		(size 0.65 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 1.425 0)
		(size 0.65 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 1.425 -0.5)
		(size 0.65 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 1.425 -1)
		(size 0.65 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at 1.425 -1.5)
		(size 0.65 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 1.425 -2)
		(size 0.65 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at 0 0)
		(size 1.66 4.4)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/DFN-18-1EP_3x5mm_P0.5mm_EP1.66x4.4mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
