(footprint "DFN-20-1EP_5x6mm_P0.5mm_EP3.24x4.24mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "DFN20, 6x5, 0.5P; CASE 505AB (see ON Semiconductor 505AB.PDF)")
	(tags "DFN 0.5")
	(property "Reference" "REF**"
		(at 0 -4.075 0)
		(layer "F.SilkS")
	)
	(property "Value" "DFN-20-1EP_5x6mm_P0.5mm_EP3.24x4.24mm"
		(at 0 4.075 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -1.08 -1.59)
		(size 0.86 0.86)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.08 -0.53)
		(size 0.86 0.86)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.08 0.53)
		(size 0.86 0.86)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.08 1.59)
		(size 0.86 0.86)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 -1.59)
		(size 0.86 0.86)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 -0.53)
		(size 0.86 0.86)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 0.53)
		(size 0.86 0.86)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 1.59)
		(size 0.86 0.86)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.08 -1.59)
		(size 0.86 0.86)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.08 -0.53)
		(size 0.86 0.86)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.08 0.53)
		(size 0.86 0.86)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.08 1.59)
		(size 0.86 0.86)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -2.26 -2.25)
		(size 0.78 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -2.26 -1.75)
		(size 0.78 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -2.26 -1.25)
		(size 0.78 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -2.26 -0.75)
		(size 0.78 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -2.26 -0.25)
		(size 0.78 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -2.26 0.25)
		(size 0.78 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -2.26 0.75)
		(size 0.78 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -2.26 1.25)
		(size 0.78 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -2.26 1.75)
		(size 0.78 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -2.26 2.25)
		(size 0.78 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 2.26 2.25)
		(size 0.78 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 2.26 1.75)
		(size 0.78 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 2.26 1.25)
		(size 0.78 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 2.26 0.75)
		(size 0.78 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 2.26 0.25)
		(size 0.78 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 2.26 -0.25)
		(size 0.78 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at 2.26 -0.75)
		(size 0.78 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 2.26 -1.25)
		(size 0.78 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at 2.26 -1.75)
		(size 0.78 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 2.26 -2.25)
		(size 0.78 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at 0 0)
		(size 3.24 4.24)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/DFN-20-1EP_5x6mm_P0.5mm_EP3.24x4.24mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
