(footprint "DFN-44-1EP_5x8.9mm_P0.4mm_EP3.7x8.4mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "DFN44 8.9x5, 0.4P; CASE 506BU-01 (see ON Semiconductor 506BU.PDF)")
	(tags "DFN 0.4")
	(property "Reference" "REF**"
		(at 0 -5.525 0)
		(layer "F.SilkS")
	)
	(property "Value" "DFN-44-1EP_5x8.9mm_P0.4mm_EP3.7x8.4mm"
		(at 0 5.525 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -1.2 -3.5)
		(size 0.98 1.15)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.2 -2.1)
		(size 0.98 1.15)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.2 -0.7)
		(size 0.98 1.15)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.2 0.7)
		(size 0.98 1.15)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.2 2.1)
		(size 0.98 1.15)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.2 3.5)
		(size 0.98 1.15)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 -3.5)
		(size 0.98 1.15)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 -2.1)
		(size 0.98 1.15)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 -0.7)
		(size 0.98 1.15)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 0.7)
		(size 0.98 1.15)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 2.1)
		(size 0.98 1.15)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 3.5)
		(size 0.98 1.15)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.2 -3.5)
		(size 0.98 1.15)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.2 -2.1)
		(size 0.98 1.15)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.2 -0.7)
		(size 0.98 1.15)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.2 0.7)
		(size 0.98 1.15)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.2 2.1)
		(size 0.98 1.15)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.2 3.5)
		(size 0.98 1.15)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -2.335 -4.2)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -2.335 -3.8)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -2.335 -3.4)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -2.335 -3)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -2.335 -2.6)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -2.335 -2.2)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -2.335 -1.8)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -2.335 -1.4)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -2.335 -1)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -2.335 -0.6)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -2.335 -0.2)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -2.335 0.2)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -2.335 0.6)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -2.335 1)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -2.335 1.4)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -2.335 1.8)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -2.335 2.2)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -2.335 2.6)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -2.335 3)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at -2.335 3.4)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at -2.335 3.8)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at -2.335 4.2)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at 2.335 4.2)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 2.335 3.8)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at 2.335 3.4)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 2.335 3)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at 2.335 2.6)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 2.335 2.2)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 2.335 1.8)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at 2.335 1.4)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at 2.335 1)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at 2.335 0.6)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at 2.335 0.2)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at 2.335 -0.2)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at 2.335 -0.6)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at 2.335 -1)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at 2.335 -1.4)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at 2.335 -1.8)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at 2.335 -2.2)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd rect
		(at 2.335 -2.6)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd rect
		(at 2.335 -3)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd rect
		(at 2.335 -3.4)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd rect
		(at 2.335 -3.8)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd rect
		(at 2.335 -4.2)
		(size 0.63 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "45" smd rect
		(at 0 0)
		(size 3.7 8.4)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/DFN-44-1EP_5x8.9mm_P0.4mm_EP3.7x8.4mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
