(footprint "DFN-4_5x7mm_P5.08mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "DFN, 4 Pin (https://ww1.microchip.com/downloads/aemDocuments/documents/TCG/ProductDocuments/DataSheets/DSC1001-3-4-1.8V-3.3V-Low-Power-Precision-CMOS-Oscillators-DS20005529.pdf#page=14), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "DFN NoLead Microchip-DFN75-4LD-PL-1")
	(property "Reference" "REF**"
		(at 0 -4.45 0)
		(layer "F.SilkS")
	)
	(property "Value" "DFN-4_5x7mm_P5.08mm"
		(at 0 4.45 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -2.0375 -2.54)
		(size 1.675 1.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.178571)
	)
	(pad "2" smd roundrect
		(at -2.0375 2.54)
		(size 1.675 1.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.178571)
	)
	(pad "3" smd roundrect
		(at 2.0375 2.54)
		(size 1.675 1.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.178571)
	)
	(pad "4" smd roundrect
		(at 2.0375 -2.54)
		(size 1.675 1.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.178571)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu")
		(name "Keepout")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(filled_areas_thickness no)
		(min_thickness 0.25)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(copperpour not_allowed)
			(pads allowed)
			(footprints allowed)
		)
		(fill)
		(polygon
			(pts
				(xy -1.9 -1.25)
				(xy 1.9 -1.25)
				(xy 1.9 1.25)
				(xy -1.9 1.25)
				(xy -1.9 -1.25)
			)
		)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/DFN-4_5x7mm_P5.08mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
