(footprint "DFN-6-1EP_3x3mm_P0.95mm_EP1.7x2.6mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "DFN6 3*3 MM, 0.95 PITCH; CASE 506AH-01 (see ON Semiconductor 506AH.PDF)")
	(tags "DFN 0.95")
	(property "Reference" "REF**"
		(at 0 -2.575 0)
		(layer "F.SilkS")
	)
	(property "Value" "DFN-6-1EP_3x3mm_P0.95mm_EP1.7x2.6mm"
		(at 0 2.575 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -0.425 -0.866)
		(size 0.66 0.73)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.425 0)
		(size 0.66 0.73)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.425 0.866)
		(size 0.66 0.73)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.425 -0.866)
		(size 0.66 0.73)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.425 0)
		(size 0.66 0.73)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.425 0.866)
		(size 0.66 0.73)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -1.34 -0.95)
		(size 0.63 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.34 0)
		(size 0.63 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.34 0.95)
		(size 0.63 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 1.34 0.95)
		(size 0.63 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1.34 0)
		(size 0.63 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 1.34 -0.95)
		(size 0.63 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 0 0)
		(size 1.7 2.6)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/DFN-6-1EP_3x3mm_P0.95mm_EP1.7x2.6mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
