(footprint "DFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "8-Lead Plastic Dual Flat, No Lead Package (8MA2) - 2x3x0.6 mm Body [UDFN] (see Atmel-8815-SEEPROM-AT24CS01-02-Datasheet.pdf)")
	(tags "DFN 0.5")
	(property "Reference" "REF**"
		(at 0 -2.05 0)
		(layer "F.SilkS")
	)
	(property "Value" "DFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.5mm"
		(at 0 2.05 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -0.325 -0.375)
		(size 0.5 0.6)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.325 0.375)
		(size 0.5 0.6)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.325 -0.375)
		(size 0.5 0.6)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.325 0.375)
		(size 0.5 0.6)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -1.45 -0.75)
		(size 0.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.45 -0.25)
		(size 0.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.45 0.25)
		(size 0.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.45 0.75)
		(size 0.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1.45 0.75)
		(size 0.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 1.45 0.25)
		(size 0.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 1.45 -0.25)
		(size 0.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 1.45 -0.75)
		(size 0.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 0 0)
		(size 1.3 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/DFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
