(footprint "DFN-8-1EP_6x5mm_P1.27mm_EP2x2mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "DD Package; 8-Lead Plastic DFN (6mm x 5mm) (see http://www.everspin.com/file/236/download)")
	(tags "dfn ")
	(property "Reference" "REF**"
		(at 0 -3.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "DFN-8-1EP_6x5mm_P1.27mm_EP2x2mm"
		(at 0 3.65 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -0.5 -0.5 270)
		(size 0.8 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.5 0.5 270)
		(size 0.8 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.5 -0.5 270)
		(size 0.8 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.5 0.5 270)
		(size 0.8 0.8)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -2.9 -1.905 270)
		(size 0.5 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -2.9 -0.635 270)
		(size 0.5 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -2.9 0.635 270)
		(size 0.5 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -2.9 1.905 270)
		(size 0.5 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 2.9 1.905 270)
		(size 0.5 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 2.9 0.635 270)
		(size 0.5 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 2.9 -0.635 270)
		(size 0.5 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 2.9 -1.905 270)
		(size 0.5 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 0 0 270)
		(size 2 2)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/DFN-8-1EP_6x5mm_P1.27mm_EP2x2mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
