(footprint "DFN-S-8-1EP_6x5mm_P1.27mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "8-Lead Plastic Dual Flat, No Lead Package (MF) - 6x5 mm Body [DFN-S] (see Microchip Packaging Specification 00000049BS.pdf)")
	(tags "DFN 1.27")
	(property "Reference" "REF**"
		(at 0 -3.575 0)
		(layer "F.SilkS")
	)
	(property "Value" "DFN-S-8-1EP_6x5mm_P1.27mm"
		(at 0 3.575 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd oval
		(at -2.8 -1.905)
		(size 1.1 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd oval
		(at -2.8 -0.635)
		(size 1.1 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd oval
		(at -2.8 0.635)
		(size 1.1 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd oval
		(at -2.8 1.905)
		(size 1.1 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd oval
		(at 2.8 1.905)
		(size 1.1 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd oval
		(at 2.8 0.635)
		(size 1.1 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd oval
		(at 2.8 -0.635)
		(size 1.1 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd oval
		(at 2.8 -1.905)
		(size 1.1 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -0.6 -1.5375)
		(size 1.2 1.025)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio -0.2)
	)
	(pad "9" smd rect
		(at -0.6 -0.5125)
		(size 1.2 1.025)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio -0.2)
	)
	(pad "9" smd rect
		(at -0.6 0.512499)
		(size 1.2 1.025)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio -0.2)
	)
	(pad "9" smd rect
		(at -0.6 1.5375)
		(size 1.2 1.025)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio -0.2)
	)
	(pad "9" smd rect
		(at 0.6 -1.5375)
		(size 1.2 1.025)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio -0.2)
	)
	(pad "9" smd rect
		(at 0.6 -0.5125)
		(size 1.2 1.025)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio -0.2)
	)
	(pad "9" smd rect
		(at 0.6 0.512499)
		(size 1.2 1.025)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio -0.2)
	)
	(pad "9" smd rect
		(at 0.6 1.5375)
		(size 1.2 1.025)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio -0.2)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/DFN-S-8-1EP_6x5mm_P1.27mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
