(footprint "EPC_QFN-13-3EP_3.5x5mm_P0.5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "EPC QFN-13, 5.0x3.5mm, Pitch 0.5mm, https://epc-co.com/epc/Portals/0/epc/documents/datasheets/EPC23102_datasheet.pdf")
	(tags "ePower-Stage-IC EPC23102 EPC23103 EPC23104")
	(property "Reference" "REF**"
		(at 0 -3.25 0)
		(layer "F.SilkS")
	)
	(property "Value" "EPC_QFN-13-3EP_3.5x5mm_P0.5mm"
		(at 0 3 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(net_tie_pad_groups "7,8")
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -2.598 -1.428)
		(size 0.305 0.4)
		(layers "F.Paste")
		(roundrect_rratio 0.1639344262)
	)
	(pad "" smd roundrect
		(at -2.438 1.435 180)
		(size 0.625 0.325)
		(layers "F.Paste")
		(roundrect_rratio 0.1538461538)
	)
	(pad "" smd roundrect
		(at -2.3625 -1.428 180)
		(size 0.675 0.3)
		(layers "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "" smd roundrect
		(at -2.351 -0.575 180)
		(size 0.8 0.24)
		(layers "F.Paste")
		(roundrect_rratio 0.2083333333)
	)
	(pad "" smd roundrect
		(at -2.351 -0.078 180)
		(size 0.8 0.24)
		(layers "F.Paste")
		(roundrect_rratio 0.2083333333)
	)
	(pad "" smd roundrect
		(at -2.351 0.422 180)
		(size 0.8 0.24)
		(layers "F.Paste")
		(roundrect_rratio 0.2083333333)
	)
	(pad "" smd roundrect
		(at -2.351 0.922 180)
		(size 0.8 0.24)
		(layers "F.Paste")
		(roundrect_rratio 0.2083333333)
	)
	(pad "" smd roundrect
		(at -2.325 -0.578 180)
		(size 0.75 0.3)
		(layers "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "" smd roundrect
		(at -2.325 -0.078 180)
		(size 0.75 0.3)
		(layers "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "" smd roundrect
		(at -2.325 0.422 180)
		(size 0.75 0.3)
		(layers "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "" smd roundrect
		(at -2.325 0.922 180)
		(size 0.75 0.3)
		(layers "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "" smd roundrect
		(at -2.1875 1.422 180)
		(size 1.025 0.3)
		(layers "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "" smd roundrect
		(at -2.175 -1.615 90)
		(size 0.675 0.3)
		(layers "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "" smd roundrect
		(at -2.145 -1.603 270)
		(size 0.8 0.24)
		(layers "F.Paste")
		(roundrect_rratio 0.2083333333)
	)
	(pad "" smd roundrect
		(at -1.825 1.61 90)
		(size 0.675 0.3)
		(layers "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "" smd roundrect
		(at -1.825 1.622 270)
		(size 0.7 0.24)
		(layers "F.Paste")
		(roundrect_rratio 0.2083333333)
	)
	(pad "" smd roundrect
		(at -1.675 -1.603 270)
		(size 0.8 0.24)
		(layers "F.Paste")
		(roundrect_rratio 0.2083333333)
	)
	(pad "" smd roundrect
		(at -1.675 -1.578 90)
		(size 0.75 0.3)
		(layers "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "" smd roundrect
		(at -1.325 1.572 90)
		(size 0.75 0.3)
		(layers "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "" smd roundrect
		(at -1.325 1.598 270)
		(size 0.8 0.24)
		(layers "F.Paste")
		(roundrect_rratio 0.2083333333)
	)
	(pad "" smd roundrect
		(at -1.175 -1.603 270)
		(size 0.8 0.24)
		(layers "F.Paste")
		(roundrect_rratio 0.2083333333)
	)
	(pad "" smd roundrect
		(at -1.175 -1.578 90)
		(size 0.75 0.3)
		(layers "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "" smd roundrect
		(at -0.825 1.572 90)
		(size 0.75 0.3)
		(layers "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "" smd roundrect
		(at -0.825 1.598 270)
		(size 0.8 0.24)
		(layers "F.Paste")
		(roundrect_rratio 0.2083333333)
	)
	(pad "" smd roundrect
		(at -0.375 0)
		(size 1 0.355)
		(layers "F.Paste")
		(roundrect_rratio 0.1408450704)
	)
	(pad "" smd roundrect
		(at -0.375 1.81)
		(size 0.32 0.33)
		(layers "F.Paste")
		(roundrect_rratio 0.15625)
	)
	(pad "" smd roundrect
		(at -0.325 -1.81)
		(size 0.32 0.33)
		(layers "F.Paste")
		(roundrect_rratio 0.15625)
	)
	(pad "" smd roundrect
		(at 0.021 -1.215)
		(size 1 0.495)
		(layers "F.Paste")
		(roundrect_rratio 0.101010101)
	)
	(pad "" smd roundrect
		(at 0.021 1.215)
		(size 1 0.495)
		(layers "F.Paste")
		(roundrect_rratio 0.101010101)
	)
	(pad "" smd roundrect
		(at 0.125 1.81)
		(size 0.32 0.33)
		(layers "F.Paste")
		(roundrect_rratio 0.15625)
	)
	(pad "" smd roundrect
		(at 0.175 -1.81)
		(size 0.32 0.33)
		(layers "F.Paste")
		(roundrect_rratio 0.15625)
	)
	(pad "" smd roundrect
		(at 0.625 1.81)
		(size 0.32 0.33)
		(layers "F.Paste")
		(roundrect_rratio 0.15625)
	)
	(pad "" smd roundrect
		(at 0.675 -1.81)
		(size 0.32 0.33)
		(layers "F.Paste")
		(roundrect_rratio 0.15625)
	)
	(pad "" smd roundrect
		(at 0.863 0 180)
		(size 3.675 0.48)
		(layers "F.Mask")
		(roundrect_rratio 0.21875)
	)
	(pad "" smd roundrect
		(at 1.005 0)
		(size 1 0.355)
		(layers "F.Paste")
		(roundrect_rratio 0.1408450704)
	)
	(pad "" smd roundrect
		(at 1.1 -1.428 180)
		(size 3.2 1.05)
		(layers "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "" smd roundrect
		(at 1.1 1.422 180)
		(size 3.2 1.05)
		(layers "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "" smd roundrect
		(at 1.125 1.81)
		(size 0.32 0.33)
		(layers "F.Paste")
		(roundrect_rratio 0.15625)
	)
	(pad "" smd roundrect
		(at 1.175 -1.81)
		(size 0.32 0.33)
		(layers "F.Paste")
		(roundrect_rratio 0.15625)
	)
	(pad "" smd roundrect
		(at 1.201 -1.215)
		(size 1 0.495)
		(layers "F.Paste")
		(roundrect_rratio 0.101010101)
	)
	(pad "" smd roundrect
		(at 1.201 1.215)
		(size 1 0.495)
		(layers "F.Paste")
		(roundrect_rratio 0.101010101)
	)
	(pad "" smd roundrect
		(at 1.625 1.81)
		(size 0.32 0.33)
		(layers "F.Paste")
		(roundrect_rratio 0.15625)
	)
	(pad "" smd roundrect
		(at 1.675 -1.81)
		(size 0.32 0.33)
		(layers "F.Paste")
		(roundrect_rratio 0.15625)
	)
	(pad "" smd roundrect
		(at 2.125 1.81)
		(size 0.32 0.33)
		(layers "F.Paste")
		(roundrect_rratio 0.15625)
	)
	(pad "" smd roundrect
		(at 2.175 -1.81)
		(size 0.32 0.33)
		(layers "F.Paste")
		(roundrect_rratio 0.15625)
	)
	(pad "" smd roundrect
		(at 2.29 -1.215)
		(size 0.819 0.495)
		(layers "F.Paste")
		(roundrect_rratio 0.101010101)
	)
	(pad "" smd roundrect
		(at 2.29 0)
		(size 0.815 0.355)
		(layers "F.Paste")
		(roundrect_rratio 0.1408450704)
	)
	(pad "" smd roundrect
		(at 2.29 1.215)
		(size 0.819 0.495)
		(layers "F.Paste")
		(roundrect_rratio 0.101010101)
	)
	(pad "1" smd roundrect
		(at -2.351 -0.578)
		(size 0.9 0.35)
		(layers "F.Cu")
		(roundrect_rratio 0.2285714286)
	)
	(pad "2" smd roundrect
		(at -2.351 -0.078)
		(size 0.9 0.35)
		(layers "F.Cu")
		(roundrect_rratio 0.2285714286)
	)
	(pad "3" smd roundrect
		(at -2.351 0.422)
		(size 0.9 0.35)
		(layers "F.Cu")
		(roundrect_rratio 0.2285714286)
	)
	(pad "4" smd roundrect
		(at -2.351 0.922)
		(size 0.9 0.35)
		(layers "F.Cu")
		(roundrect_rratio 0.2285714286)
	)
	(pad "5" smd roundrect
		(at -2.225 1.647)
		(size 1.15 0.8)
		(layers "F.Cu")
		(roundrect_rratio 0.1)
	)
	(pad "6" smd roundrect
		(at -1.325 1.598 90)
		(size 0.9 0.35)
		(layers "F.Cu")
		(roundrect_rratio 0.2285714286)
	)
	(pad "7" smd roundrect
		(at -0.825 1.598 90)
		(size 0.9 0.35)
		(layers "F.Cu")
		(roundrect_rratio 0.2285714286)
	)
	(pad "8" smd roundrect
		(at 0.898 1.447)
		(size 3.8 1.2)
		(layers "F.Cu")
		(roundrect_rratio 0.06666666667)
	)
	(pad "9" smd roundrect
		(at -0.9255 0)
		(size 0.25 0.623)
		(layers "F.Cu")
		(roundrect_rratio 0.32)
	)
	(pad "9" smd roundrect
		(at 0.937 0.107)
		(size 3.725 1.22)
		(layers "F.Cu")
		(roundrect_rratio 0.06557377049)
	)
	(pad "10" smd roundrect
		(at 1.125 -1.39)
		(size 3.35 1.39)
		(layers "F.Cu")
		(roundrect_rratio 0.05755395683)
	)
	(pad "11" smd roundrect
		(at -1.175 -1.603 90)
		(size 0.9 0.35)
		(layers "F.Cu")
		(roundrect_rratio 0.2285714286)
	)
	(pad "12" smd roundrect
		(at -1.675 -1.603 90)
		(size 0.9 0.35)
		(layers "F.Cu")
		(roundrect_rratio 0.2285714286)
	)
	(pad "13" smd roundrect
		(at -2.4 -1.603)
		(size 0.8 0.9)
		(layers "F.Cu")
		(roundrect_rratio 0.1)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/EPC_QFN-13-3EP_3.5x5mm_P0.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
