(footprint "HVQFN-24-1EP_4x4mm_P0.5mm_EP2.5x2.5mm_ThermalVias"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "HVQFN, 24 Pin (https://www.nxp.com/docs/en/package-information/SOT616-3.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "HVQFN NoLead")
	(property "Reference" "REF**"
		(at 0 -3.33 0)
		(layer "F.SilkS")
	)
	(property "Value" "HVQFN-24-1EP_4x4mm_P0.5mm_EP2.5x2.5mm_ThermalVias"
		(at 0 3.33 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at -0.5 -0.5)
		(size 0.778626 0.778626)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.315114 -0.192176)
					(xy -0.192176 -0.315114)
					(xy 0.192176 -0.315114)
					(xy 0.315114 -0.192176)
					(xy 0.315114 0.192176)
					(xy 0.192176 0.315114)
					(xy -0.192176 0.315114)
					(xy -0.315114 0.192176)
				)
				(width 0.296797)
			)
		)
	)
	(pad "" smd custom
		(at -0.5 0.5)
		(size 0.778626 0.778626)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.315114 -0.192176)
					(xy -0.192176 -0.315114)
					(xy 0.192176 -0.315114)
					(xy 0.315114 -0.192176)
					(xy 0.315114 0.192176)
					(xy 0.192176 0.315114)
					(xy -0.192176 0.315114)
					(xy -0.315114 0.192176)
				)
				(width 0.296797)
			)
		)
	)
	(pad "" smd custom
		(at 0.5 -0.5)
		(size 0.778626 0.778626)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.315114 -0.192176)
					(xy -0.192176 -0.315114)
					(xy 0.192176 -0.315114)
					(xy 0.315114 -0.192176)
					(xy 0.315114 0.192176)
					(xy 0.192176 0.315114)
					(xy -0.192176 0.315114)
					(xy -0.315114 0.192176)
				)
				(width 0.296797)
			)
		)
	)
	(pad "" smd custom
		(at 0.5 0.5)
		(size 0.778626 0.778626)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.315114 -0.192176)
					(xy -0.192176 -0.315114)
					(xy 0.192176 -0.315114)
					(xy 0.315114 -0.192176)
					(xy 0.315114 0.192176)
					(xy 0.192176 0.315114)
					(xy -0.192176 0.315114)
					(xy -0.315114 0.192176)
				)
				(width 0.296797)
			)
		)
	)
	(pad "1" smd roundrect
		(at -1.9375 -1.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -1.9375 -0.75)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -1.9375 -0.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -1.9375 0.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -1.9375 0.75)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -1.9375 1.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -1.25 1.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -0.75 1.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -0.25 1.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at 0.25 1.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at 0.75 1.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at 1.25 1.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 1.9375 1.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at 1.9375 0.75)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at 1.9375 0.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at 1.9375 -0.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at 1.9375 -0.75)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at 1.9375 -1.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at 1.25 -1.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at 0.75 -1.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at 0.25 -1.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at -0.25 -1.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at -0.75 -1.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at -1.25 -1.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "25" thru_hole circle
		(at -1 -1)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole circle
		(at -1 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole circle
		(at -1 1)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole circle
		(at 0 -1)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole circle
		(at 0 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "25" smd rect
		(at 0 0)
		(size 2.5 2.5)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(pad "25" smd rect
		(at 0 0)
		(size 2.5 2.5)
		(property pad_prop_heatsink)
		(layers "B.Cu")
		(zone_connect 2)
	)
	(pad "25" thru_hole circle
		(at 0 1)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole circle
		(at 1 -1)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole circle
		(at 1 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole circle
		(at 1 1)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/HVQFN-24-1EP_4x4mm_P0.5mm_EP2.5x2.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
