(footprint "Infineon_MLPQ-16-14-1EP_4x4mm_P0.5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "MLPQ 32 leads, 7x7mm, 0.127mm stencil (https://www.infineon.com/dgdl/Infineon-AN1170-AN-v05_00-EN.pdf?fileId=5546d462533600a40153559ac3e51134)")
	(tags "mlpq 32 7x7mm")
	(property "Reference" "REF**"
		(at 0 -3.3 0)
		(layer "F.SilkS")
	)
	(property "Value" "Infineon_MLPQ-16-14-1EP_4x4mm_P0.5mm"
		(at 0 3.3 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(solder_paste_margin -0.02)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -0.335 -0.105)
		(size 1.5 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.335 0.835)
		(size 1.5 0.8)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -1.975 -0.75)
		(size 0.65 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.02)
	)
	(pad "2" smd rect
		(at -1.975 -0.25)
		(size 0.65 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.02)
	)
	(pad "3" smd rect
		(at -1.975 0.25)
		(size 0.65 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.02)
	)
	(pad "4" smd rect
		(at -1.975 0.75)
		(size 0.65 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.02)
	)
	(pad "5" smd rect
		(at -0.75 1.975)
		(size 0.22 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.02)
	)
	(pad "6" smd rect
		(at -0.25 1.975)
		(size 0.22 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.02)
	)
	(pad "7" smd rect
		(at 0.25 1.975)
		(size 0.22 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.02)
	)
	(pad "8" smd rect
		(at 0.75 1.975)
		(size 0.22 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.02)
	)
	(pad "9" smd rect
		(at 1.975 0.75)
		(size 0.65 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.02)
	)
	(pad "11" smd rect
		(at 1.975 -0.25)
		(size 0.65 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.02)
	)
	(pad "12" smd rect
		(at 1.975 -0.75)
		(size 0.65 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.02)
	)
	(pad "13" smd rect
		(at 0.75 -1.975)
		(size 0.22 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.02)
	)
	(pad "14" smd rect
		(at 0.25 -1.975)
		(size 0.22 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.02)
	)
	(pad "16" smd rect
		(at -0.75 -1.975)
		(size 0.22 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.02)
	)
	(pad "17" smd rect
		(at -1.075 -0.375 45)
		(size 0.2828 0.2828)
		(layers "F.Cu" "F.Mask")
	)
	(pad "17" smd rect
		(at -0.335 0.465)
		(size 1.88 1.68)
		(layers "F.Cu" "F.Mask")
	)
	(pad "17" smd rect
		(at -0.235 -0.475)
		(size 1.68 0.2)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Infineon_MLPQ-16-14-1EP_4x4mm_P0.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
