(footprint "Infineon_MLPQ-40-32-1EP_7x7mm_P0.5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "MLPQ 32 leads, 7x7mm, 0.127mm stencil (https://www.infineon.com/dgdl/Infineon-AN1170-AN-v05_00-EN.pdf?fileId=5546d462533600a40153559ac3e51134)")
	(tags "mlpq 32 7x7mm")
	(property "Reference" "REF**"
		(at 0 -4.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "Infineon_MLPQ-40-32-1EP_7x7mm_P0.5mm"
		(at 0 4.8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -3.425 -2.25)
		(size 0.65 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.425 -1.75)
		(size 0.65 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.425 -1.25)
		(size 0.65 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.425 -0.75)
		(size 0.65 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.425 -0.25)
		(size 0.65 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.425 0.25)
		(size 0.65 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.425 0.75)
		(size 0.65 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.425 1.25)
		(size 0.65 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.425 1.75)
		(size 0.65 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.425 2.25)
		(size 0.65 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.25 -3.425)
		(size 0.22 0.65)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.25 3.425)
		(size 0.22 0.65)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.7955 -1.4)
		(size 1.2 1.1)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.7955 0)
		(size 1.2 1.1)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.7955 1.4)
		(size 1.2 1.1)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.75 -3.425)
		(size 0.22 0.65)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.75 3.425)
		(size 0.22 0.65)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.2375 -1.4)
		(size 1.2 1.1)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.2375 0)
		(size 1.2 1.1)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.2375 1.4)
		(size 1.2 1.1)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.25 -3.425)
		(size 0.22 0.65)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.25 3.425)
		(size 0.22 0.65)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.75 -3.425)
		(size 0.22 0.65)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.75 3.425)
		(size 0.22 0.65)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.25 -3.425)
		(size 0.22 0.65)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.25 3.425)
		(size 0.22 0.65)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.3205 -1.4)
		(size 1.2 1.1)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.3205 0)
		(size 1.2 1.1)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.3205 1.4)
		(size 1.2 1.1)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.75 -3.425)
		(size 0.22 0.65)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.75 3.425)
		(size 0.22 0.65)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 3.425 -2.25)
		(size 0.65 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 3.425 -1.75)
		(size 0.65 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 3.425 -1.25)
		(size 0.65 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 3.425 -0.75)
		(size 0.65 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 3.425 -0.25)
		(size 0.65 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 3.425 0.25)
		(size 0.65 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 3.425 0.75)
		(size 0.65 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 3.425 1.25)
		(size 0.65 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 3.425 1.75)
		(size 0.65 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 3.425 2.25)
		(size 0.65 0.22)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -3.44 -2.25)
		(size 0.7 0.24)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" smd rect
		(at -3.44 -1.75)
		(size 0.7 0.24)
		(layers "F.Cu" "F.Mask")
	)
	(pad "3" smd rect
		(at -3.44 -1.25)
		(size 0.7 0.24)
		(layers "F.Cu" "F.Mask")
	)
	(pad "4" smd rect
		(at -3.44 -0.75)
		(size 0.7 0.24)
		(layers "F.Cu" "F.Mask")
	)
	(pad "5" smd rect
		(at -3.44 -0.25)
		(size 0.7 0.24)
		(layers "F.Cu" "F.Mask")
	)
	(pad "6" smd rect
		(at -3.44 0.25)
		(size 0.7 0.24)
		(layers "F.Cu" "F.Mask")
	)
	(pad "7" smd rect
		(at -3.44 0.75)
		(size 0.7 0.24)
		(layers "F.Cu" "F.Mask")
	)
	(pad "8" smd rect
		(at -3.44 1.25)
		(size 0.7 0.24)
		(layers "F.Cu" "F.Mask")
	)
	(pad "9" smd rect
		(at -3.44 1.75)
		(size 0.7 0.24)
		(layers "F.Cu" "F.Mask")
	)
	(pad "10" smd rect
		(at -3.44 2.25)
		(size 0.7 0.24)
		(layers "F.Cu" "F.Mask")
	)
	(pad "11" smd rect
		(at -2.25 3.44)
		(size 0.24 0.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "12" smd rect
		(at -1.75 3.44)
		(size 0.24 0.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "13" smd rect
		(at 0.25 3.44)
		(size 0.24 0.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "14" smd rect
		(at 0.75 3.44)
		(size 0.24 0.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "15" smd rect
		(at 1.25 3.44)
		(size 0.24 0.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "16" smd rect
		(at 1.75 3.44)
		(size 0.24 0.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "17" smd rect
		(at 3.44 2.25)
		(size 0.7 0.24)
		(layers "F.Cu" "F.Mask")
	)
	(pad "18" smd rect
		(at 3.44 1.75)
		(size 0.7 0.24)
		(layers "F.Cu" "F.Mask")
	)
	(pad "19" smd rect
		(at 3.44 1.25)
		(size 0.7 0.24)
		(layers "F.Cu" "F.Mask")
	)
	(pad "20" smd rect
		(at 3.44 0.75)
		(size 0.7 0.24)
		(layers "F.Cu" "F.Mask")
	)
	(pad "21" smd rect
		(at 3.44 0.25)
		(size 0.7 0.24)
		(layers "F.Cu" "F.Mask")
	)
	(pad "22" smd rect
		(at 3.44 -0.25)
		(size 0.7 0.24)
		(layers "F.Cu" "F.Mask")
	)
	(pad "23" smd rect
		(at 3.44 -0.75)
		(size 0.7 0.24)
		(layers "F.Cu" "F.Mask")
	)
	(pad "24" smd rect
		(at 3.44 -1.25)
		(size 0.7 0.24)
		(layers "F.Cu" "F.Mask")
	)
	(pad "25" smd rect
		(at 3.44 -1.75)
		(size 0.7 0.24)
		(layers "F.Cu" "F.Mask")
	)
	(pad "26" smd rect
		(at 3.44 -2.25)
		(size 0.7 0.24)
		(layers "F.Cu" "F.Mask")
	)
	(pad "27" smd rect
		(at 1.75 -3.44)
		(size 0.24 0.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "28" smd rect
		(at 1.25 -3.44)
		(size 0.24 0.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "29" smd rect
		(at 0.75 -3.44)
		(size 0.24 0.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "30" smd rect
		(at 0.25 -3.44)
		(size 0.24 0.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "31" smd rect
		(at -1.75 -3.44)
		(size 0.24 0.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "32" smd rect
		(at -2.25 -3.44)
		(size 0.24 0.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "33" smd rect
		(at -2.225 -1.75 45)
		(size 0.495 0.495)
		(layers "F.Cu" "F.Mask")
	)
	(pad "33" smd rect
		(at -0.2375 0.175)
		(size 4.675 3.85)
		(layers "F.Cu" "F.Mask")
	)
	(pad "33" smd rect
		(at -0.0625 -1.925)
		(size 4.325 0.35)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Infineon_MLPQ-40-32-1EP_7x7mm_P0.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
