(footprint "Infineon_MLPQ-48-1EP_7x7mm_P0.5mm_EP5.55x5.55mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "MLPQ 48 leads, 7x7mm (https://www.infineon.com/dgdl/irs2093mpbf.pdf?fileId=5546d462533600a401535675fb892793)")
	(tags "mlpq 32 7x7mm")
	(property "Reference" "REF**"
		(at 0 -4.7 0)
		(layer "F.SilkS")
	)
	(property "Value" "Infineon_MLPQ-48-1EP_7x7mm_P0.5mm_EP5.55x5.55mm"
		(at 0 4.7 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -3.425 -2.75)
		(size 0.55 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.425 -2.25)
		(size 0.55 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.425 -1.75)
		(size 0.55 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.425 -1.25)
		(size 0.55 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.425 -0.75)
		(size 0.55 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.425 -0.25)
		(size 0.55 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.425 0.25)
		(size 0.55 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.425 0.75)
		(size 0.55 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.425 1.25)
		(size 0.55 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.425 1.75)
		(size 0.55 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.425 2.25)
		(size 0.55 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.425 2.75)
		(size 0.55 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.75 -3.425)
		(size 0.22 0.55)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.75 3.425)
		(size 0.22 0.55)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.25 -3.425)
		(size 0.22 0.55)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.25 3.425)
		(size 0.22 0.55)
		(layers "F.Paste")
	)
	(pad "" smd custom
		(at -2.175 -2.175)
		(size 0.5 0.5)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.55 0.55) (xy -0.55 0.55) (xy -0.55 -0.211) (xy -0.211 -0.55) (xy 0.55 -0.55)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd rect
		(at -2.175 -0.725)
		(size 1.1 1.1)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.175 0.725)
		(size 1.1 1.1)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.175 2.175)
		(size 1.1 1.1)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.75 -3.425)
		(size 0.22 0.55)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.75 3.425)
		(size 0.22 0.55)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.25 -3.425)
		(size 0.22 0.55)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.25 3.425)
		(size 0.22 0.55)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.75 -3.425)
		(size 0.22 0.55)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.75 3.425)
		(size 0.22 0.55)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.725 -2.175)
		(size 1.1 1.1)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.725 -0.725)
		(size 1.1 1.1)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.725 0.725)
		(size 1.1 1.1)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.725 2.175)
		(size 1.1 1.1)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.25 -3.425)
		(size 0.22 0.55)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.25 3.425)
		(size 0.22 0.55)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.25 -3.425)
		(size 0.22 0.55)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.25 3.425)
		(size 0.22 0.55)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.725 -2.175)
		(size 1.1 1.1)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.725 -0.725)
		(size 1.1 1.1)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.725 0.725)
		(size 1.1 1.1)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.725 2.175)
		(size 1.1 1.1)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.75 -3.425)
		(size 0.22 0.55)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.75 3.425)
		(size 0.22 0.55)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.25 -3.425)
		(size 0.22 0.55)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.25 3.425)
		(size 0.22 0.55)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.75 -3.425)
		(size 0.22 0.55)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.75 3.425)
		(size 0.22 0.55)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 2.175 -2.175)
		(size 1.1 1.1)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 2.175 -0.725)
		(size 1.1 1.1)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 2.175 0.725)
		(size 1.1 1.1)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 2.175 2.175)
		(size 1.1 1.1)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 2.25 -3.425)
		(size 0.22 0.55)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 2.25 3.425)
		(size 0.22 0.55)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 2.75 -3.425)
		(size 0.22 0.55)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 2.75 3.425)
		(size 0.22 0.55)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 3.425 -2.75)
		(size 0.55 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 3.425 -2.25)
		(size 0.55 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 3.425 -1.75)
		(size 0.55 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 3.425 -1.25)
		(size 0.55 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 3.425 -0.75)
		(size 0.55 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 3.425 -0.25)
		(size 0.55 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 3.425 0.25)
		(size 0.55 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 3.425 0.75)
		(size 0.55 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 3.425 1.25)
		(size 0.55 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 3.425 1.75)
		(size 0.55 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 3.425 2.25)
		(size 0.55 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 3.425 2.75)
		(size 0.55 0.22)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -3.425 -2.75)
		(size 0.65 0.22)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" smd rect
		(at -3.425 -2.25)
		(size 0.65 0.22)
		(layers "F.Cu" "F.Mask")
	)
	(pad "3" smd rect
		(at -3.425 -1.75)
		(size 0.65 0.22)
		(layers "F.Cu" "F.Mask")
	)
	(pad "4" smd rect
		(at -3.425 -1.25)
		(size 0.65 0.22)
		(layers "F.Cu" "F.Mask")
	)
	(pad "5" smd rect
		(at -3.425 -0.75)
		(size 0.65 0.22)
		(layers "F.Cu" "F.Mask")
	)
	(pad "6" smd rect
		(at -3.425 -0.25)
		(size 0.65 0.22)
		(layers "F.Cu" "F.Mask")
	)
	(pad "7" smd rect
		(at -3.425 0.25)
		(size 0.65 0.22)
		(layers "F.Cu" "F.Mask")
	)
	(pad "8" smd rect
		(at -3.425 0.75)
		(size 0.65 0.22)
		(layers "F.Cu" "F.Mask")
	)
	(pad "9" smd rect
		(at -3.425 1.25)
		(size 0.65 0.22)
		(layers "F.Cu" "F.Mask")
	)
	(pad "10" smd rect
		(at -3.425 1.75)
		(size 0.65 0.22)
		(layers "F.Cu" "F.Mask")
	)
	(pad "11" smd rect
		(at -3.425 2.25)
		(size 0.65 0.22)
		(layers "F.Cu" "F.Mask")
	)
	(pad "12" smd rect
		(at -3.425 2.75)
		(size 0.65 0.22)
		(layers "F.Cu" "F.Mask")
	)
	(pad "13" smd rect
		(at -2.75 3.425)
		(size 0.22 0.65)
		(layers "F.Cu" "F.Mask")
	)
	(pad "14" smd rect
		(at -2.25 3.425)
		(size 0.22 0.65)
		(layers "F.Cu" "F.Mask")
	)
	(pad "15" smd rect
		(at -1.75 3.425)
		(size 0.22 0.65)
		(layers "F.Cu" "F.Mask")
	)
	(pad "16" smd rect
		(at -1.25 3.425)
		(size 0.22 0.65)
		(layers "F.Cu" "F.Mask")
	)
	(pad "17" smd rect
		(at -0.75 3.425)
		(size 0.22 0.65)
		(layers "F.Cu" "F.Mask")
	)
	(pad "18" smd rect
		(at -0.25 3.425)
		(size 0.22 0.65)
		(layers "F.Cu" "F.Mask")
	)
	(pad "19" smd rect
		(at 0.25 3.425)
		(size 0.22 0.65)
		(layers "F.Cu" "F.Mask")
	)
	(pad "20" smd rect
		(at 0.75 3.425)
		(size 0.22 0.65)
		(layers "F.Cu" "F.Mask")
	)
	(pad "21" smd rect
		(at 1.25 3.425)
		(size 0.22 0.65)
		(layers "F.Cu" "F.Mask")
	)
	(pad "22" smd rect
		(at 1.75 3.425)
		(size 0.22 0.65)
		(layers "F.Cu" "F.Mask")
	)
	(pad "23" smd rect
		(at 2.25 3.425)
		(size 0.22 0.65)
		(layers "F.Cu" "F.Mask")
	)
	(pad "24" smd rect
		(at 2.75 3.425)
		(size 0.22 0.65)
		(layers "F.Cu" "F.Mask")
	)
	(pad "25" smd rect
		(at 3.425 2.75)
		(size 0.65 0.22)
		(layers "F.Cu" "F.Mask")
	)
	(pad "26" smd rect
		(at 3.425 2.25)
		(size 0.65 0.22)
		(layers "F.Cu" "F.Mask")
	)
	(pad "27" smd rect
		(at 3.425 1.75)
		(size 0.65 0.22)
		(layers "F.Cu" "F.Mask")
	)
	(pad "28" smd rect
		(at 3.425 1.25)
		(size 0.65 0.22)
		(layers "F.Cu" "F.Mask")
	)
	(pad "29" smd rect
		(at 3.425 0.75)
		(size 0.65 0.22)
		(layers "F.Cu" "F.Mask")
	)
	(pad "30" smd rect
		(at 3.425 0.25)
		(size 0.65 0.22)
		(layers "F.Cu" "F.Mask")
	)
	(pad "31" smd rect
		(at 3.425 -0.25)
		(size 0.65 0.22)
		(layers "F.Cu" "F.Mask")
	)
	(pad "32" smd rect
		(at 3.425 -0.75)
		(size 0.65 0.22)
		(layers "F.Cu" "F.Mask")
	)
	(pad "33" smd rect
		(at 3.425 -1.25)
		(size 0.65 0.22)
		(layers "F.Cu" "F.Mask")
	)
	(pad "34" smd rect
		(at 3.425 -1.75)
		(size 0.65 0.22)
		(layers "F.Cu" "F.Mask")
	)
	(pad "35" smd rect
		(at 3.425 -2.25)
		(size 0.65 0.22)
		(layers "F.Cu" "F.Mask")
	)
	(pad "36" smd rect
		(at 3.425 -2.75)
		(size 0.65 0.22)
		(layers "F.Cu" "F.Mask")
	)
	(pad "37" smd rect
		(at 2.75 -3.425)
		(size 0.22 0.65)
		(layers "F.Cu" "F.Mask")
	)
	(pad "38" smd rect
		(at 2.25 -3.425)
		(size 0.22 0.65)
		(layers "F.Cu" "F.Mask")
	)
	(pad "39" smd rect
		(at 1.75 -3.425)
		(size 0.22 0.65)
		(layers "F.Cu" "F.Mask")
	)
	(pad "40" smd rect
		(at 1.25 -3.425)
		(size 0.22 0.65)
		(layers "F.Cu" "F.Mask")
	)
	(pad "41" smd rect
		(at 0.75 -3.425)
		(size 0.22 0.65)
		(layers "F.Cu" "F.Mask")
	)
	(pad "42" smd rect
		(at 0.25 -3.425)
		(size 0.22 0.65)
		(layers "F.Cu" "F.Mask")
	)
	(pad "43" smd rect
		(at -0.25 -3.425)
		(size 0.22 0.65)
		(layers "F.Cu" "F.Mask")
	)
	(pad "44" smd rect
		(at -0.75 -3.425)
		(size 0.22 0.65)
		(layers "F.Cu" "F.Mask")
	)
	(pad "45" smd rect
		(at -1.25 -3.425)
		(size 0.22 0.65)
		(layers "F.Cu" "F.Mask")
	)
	(pad "46" smd rect
		(at -1.75 -3.425)
		(size 0.22 0.65)
		(layers "F.Cu" "F.Mask")
	)
	(pad "47" smd rect
		(at -2.25 -3.425)
		(size 0.22 0.65)
		(layers "F.Cu" "F.Mask")
	)
	(pad "48" smd rect
		(at -2.75 -3.425)
		(size 0.22 0.65)
		(layers "F.Cu" "F.Mask")
	)
	(pad "49" smd custom
		(at 0 0)
		(size 5 5)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 2.775 2.775) (xy -2.775 2.775) (xy -2.775 -2.407) (xy -2.407 -2.775) (xy 2.775 -2.775)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Infineon_MLPQ-48-1EP_7x7mm_P0.5mm_EP5.55x5.55mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
