(footprint "Infineon_PQFN-22-15-4EP_6x5mm_P0.65mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "PQFN 22 leads, 5x6mm, 0.127mm stencil (https://www.infineon.com/dgdl/ir4301.pdf?fileId=5546d462533600a4015355d5fc691819, https://www.infineon.com/dgdl/Infineon-AN1170-AN-v05_00-EN.pdf?fileId=5546d462533600a40153559ac3e51134)")
	(tags "pqfn 22 5x6mm")
	(property "Reference" "REF**"
		(at 0 -3.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "Infineon_PQFN-22-15-4EP_6x5mm_P0.65mm"
		(at 0 3.8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -2.8725 -1.95)
		(size 0.8 0.27)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -2.8725 -1.3)
		(size 0.8 0.27)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -2.8725 -0.65)
		(size 0.8 0.27)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -2.8725 0)
		(size 0.8 0.27)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -2.8725 0.65)
		(size 0.8 0.27)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -2.8725 1.3)
		(size 0.8 0.27)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -2.8725 1.95)
		(size 0.8 0.27)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -1.9525 -2.37)
		(size 0.27 0.8)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -1.9525 2.37)
		(size 0.27 0.8)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -1.7525 -0.795)
		(size 0.7 1.22)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -1.7525 0.695)
		(size 0.7 1.22)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -1.3025 -2.37)
		(size 0.27 0.8)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -1.3025 2.37)
		(size 0.27 0.8)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -0.9025 -0.795)
		(size 0.7 1.22)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -0.9025 0.695)
		(size 0.7 1.22)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.0605 -2.4)
		(size 0.425 0.625)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.0625 2.2205)
		(size 0.425 0.625)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.4675 0.4125)
		(size 1.24 1.78)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.5275 -1.45)
		(size 1.25 0.96)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.8355 -2.4)
		(size 0.425 0.625)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.8375 2.2205)
		(size 0.425 0.625)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.6105 -2.4)
		(size 0.425 0.625)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.6125 2.2205)
		(size 0.425 0.625)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.8475 0.4125)
		(size 1.24 1.78)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.9275 -1.45)
		(size 1.25 0.96)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 2.3855 -2.4)
		(size 0.425 0.625)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 2.3875 2.2205)
		(size 0.425 0.625)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 2.9075 -0.3275)
		(size 0.625 0.29)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 2.9075 0.4125)
		(size 0.625 0.29)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 2.9075 1.1525)
		(size 0.625 0.29)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "1" smd roundrect
		(at -2.8725 -1.95)
		(size 0.85 0.3)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -2.8725 -1.3)
		(size 0.85 0.3)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -2.8725 -0.65)
		(size 0.85 0.3)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -2.8725 0)
		(size 0.85 0.3)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -2.8725 0.65)
		(size 0.85 0.3)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -2.8725 1.3)
		(size 0.85 0.3)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -2.8725 1.95)
		(size 0.85 0.3)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -1.9525 2.375)
		(size 0.3 0.85)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -1.3025 2.375)
		(size 0.3 0.85)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd rect
		(at 0.0625 2.55)
		(size 0.425 0.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "10" smd rect
		(at 0.8375 2.55)
		(size 0.425 0.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "10" smd rect
		(at 1.225 2.025)
		(size 2.75 0.55)
		(layers "F.Cu" "F.Mask")
	)
	(pad "10" smd rect
		(at 1.6125 2.55)
		(size 0.425 0.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "10" smd rect
		(at 2.3875 2.55)
		(size 0.425 0.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "11" smd rect
		(at 1.3225 0.4125)
		(size 2.95 1.775)
		(layers "F.Cu" "F.Mask")
	)
	(pad "11" smd rect
		(at 3.0475 -0.32525)
		(size 0.5 0.2995)
		(layers "F.Cu" "F.Mask")
	)
	(pad "11" smd rect
		(at 3.0475 0.4125)
		(size 0.5 0.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "11" smd rect
		(at 3.0475 1.15025)
		(size 0.5 0.2995)
		(layers "F.Cu" "F.Mask")
	)
	(pad "12" smd rect
		(at 0.0605 -2.55)
		(size 0.425 0.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "12" smd rect
		(at 0.8355 -2.55)
		(size 0.425 0.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "12" smd rect
		(at 1.223 -1.6125)
		(size 2.75 1.375)
		(layers "F.Cu" "F.Mask")
	)
	(pad "12" smd rect
		(at 1.6105 -2.55)
		(size 0.425 0.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "12" smd rect
		(at 2.3855 -2.55)
		(size 0.425 0.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "13" smd roundrect
		(at -1.3025 -2.375)
		(size 0.3 0.85)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at -1.9525 -2.375)
		(size 0.3 0.85)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd rect
		(at -1.3305 -0.05)
		(size 1.55 2.7)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Infineon_PQFN-22-15-4EP_6x5mm_P0.65mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
