(footprint "Infineon_PQFN-44-31-5EP_7x7mm_P0.5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "PQFN 44 leads, 7x7mm, 0.127mm stencil (https://www.infineon.com/dgdl/ir4302.pdf?fileId=5546d462533600a4015355d602a9181d, https://www.infineon.com/dgdl/Infineon-AN1170-AN-v05_00-EN.pdf?fileId=5546d462533600a40153559ac3e51134)")
	(tags "pqfn 44 7x7mm")
	(property "Reference" "REF**"
		(at 0 -4.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "Infineon_PQFN-44-31-5EP_7x7mm_P0.5mm"
		(at 0 4.8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -3.3215 -2.75)
		(size 0.39 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.3215 -2.25)
		(size 0.39 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.3215 -1.75)
		(size 0.39 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.3215 -1.25)
		(size 0.39 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.3215 -0.75)
		(size 0.39 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.3215 -0.25)
		(size 0.39 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.3215 0.25)
		(size 0.39 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.3215 0.75)
		(size 0.39 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.3215 1.25)
		(size 0.39 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.3215 1.75)
		(size 0.39 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.3215 2.25)
		(size 0.39 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.3215 2.75)
		(size 0.39 0.22)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.7465 -3.325)
		(size 0.22 0.39)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.7465 3.325)
		(size 0.22 0.39)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.2465 -3.325)
		(size 0.22 0.39)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.2465 3.325)
		(size 0.22 0.39)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.2065 -1.76)
		(size 0.77 0.93)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at -2.2065 -0.52)
		(size 0.77 0.93)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at -2.2065 0.72)
		(size 0.77 0.93)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at -2.2065 1.96)
		(size 0.77 0.93)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at -1.7465 -3.015)
		(size 0.23 1.01)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.7465 3.015)
		(size 0.23 1.01)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.2465 -3.325)
		(size 0.22 0.39)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.2465 3.325)
		(size 0.22 0.39)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.1265 -1.76)
		(size 0.77 0.93)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at -1.1265 -0.52)
		(size 0.77 0.93)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at -1.1265 0.72)
		(size 0.77 0.93)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at -1.1265 1.96)
		(size 0.77 0.93)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at -0.7465 -3.325)
		(size 0.22 0.39)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.7465 3.325)
		(size 0.22 0.39)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.2465 -3.28)
		(size 0.23 0.44)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.2465 3.28)
		(size 0.23 0.44)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.0265 -3.07)
		(size 0.21 0.34)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.0265 -2.37)
		(size 0.21 0.34)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.0265 -1.67)
		(size 0.21 0.34)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.0265 1.67)
		(size 0.21 0.34)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.0265 2.37)
		(size 0.21 0.34)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.0265 3.07)
		(size 0.21 0.34)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.4735 -0.84)
		(size 0.68 0.9)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 0.4735 0.84)
		(size 0.68 0.9)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 0.7535 -3.325)
		(size 0.22 0.35)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 0.7535 3.325)
		(size 0.22 0.35)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 0.8765 -2.515)
		(size 0.65 0.9)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 0.8765 2.515)
		(size 0.65 0.9)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 1.2535 -3.325)
		(size 0.22 0.35)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 1.2535 3.325)
		(size 0.22 0.35)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 1.3835 -0.84)
		(size 0.68 0.9)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 1.3835 0.84)
		(size 0.68 0.9)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 1.7535 -3.325)
		(size 0.22 0.35)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 1.7535 3.325)
		(size 0.22 0.35)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 1.7865 -2.515)
		(size 0.65 0.9)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 1.7865 2.515)
		(size 0.65 0.9)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 2.2535 -3.325)
		(size 0.22 0.35)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 2.2535 3.325)
		(size 0.22 0.35)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 2.2935 -0.84)
		(size 0.68 0.9)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 2.2935 0.84)
		(size 0.68 0.9)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 2.6965 -2.515)
		(size 0.65 0.9)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 2.6965 2.515)
		(size 0.65 0.9)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 2.7535 -3.325)
		(size 0.22 0.35)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 2.7535 3.325)
		(size 0.22 0.35)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 3.1635 -1.3)
		(size 0.68 0.22)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 3.1635 1.3)
		(size 0.68 0.22)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 3.2835 -0.75)
		(size 0.44 0.22)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 3.2835 -0.25)
		(size 0.44 0.22)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 3.2835 0.25)
		(size 0.44 0.22)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 3.2835 0.75)
		(size 0.44 0.22)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 3.3635 -2.75)
		(size 0.28 0.22)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 3.3635 -2.25)
		(size 0.28 0.22)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 3.3635 2.25)
		(size 0.28 0.22)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 3.3635 2.75)
		(size 0.28 0.22)
		(layers "F.Mask" "F.Paste")
	)
	(pad "1" smd rect
		(at -3.4465 -2.75)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" smd rect
		(at -3.4465 -2.25)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask")
	)
	(pad "3" smd rect
		(at -3.4465 -1.75)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask")
	)
	(pad "4" smd rect
		(at -3.4465 -1.25)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask")
	)
	(pad "5" smd rect
		(at -3.4465 -0.75)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask")
	)
	(pad "6" smd rect
		(at -3.4465 -0.25)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask")
	)
	(pad "7" smd rect
		(at -3.4465 0.25)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask")
	)
	(pad "8" smd rect
		(at -3.4465 0.75)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask")
	)
	(pad "9" smd rect
		(at -3.4465 1.25)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask")
	)
	(pad "10" smd rect
		(at -3.4465 1.75)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask")
	)
	(pad "11" smd rect
		(at -3.4465 2.25)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask")
	)
	(pad "12" smd rect
		(at -3.4465 2.75)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask")
	)
	(pad "13" smd rect
		(at -2.7465 3.45)
		(size 0.25 0.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "14" smd rect
		(at -2.2465 3.45)
		(size 0.25 0.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "16" smd rect
		(at -1.2465 3.45)
		(size 0.25 0.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "17" smd rect
		(at -0.7465 3.45)
		(size 0.25 0.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "19" smd rect
		(at 0.7535 3.4775)
		(size 0.25 0.645)
		(layers "F.Cu" "F.Mask")
	)
	(pad "19" smd rect
		(at 1.2535 3.4775)
		(size 0.25 0.645)
		(layers "F.Cu" "F.Mask")
	)
	(pad "19" smd rect
		(at 1.7535 3.4775)
		(size 0.25 0.645)
		(layers "F.Cu" "F.Mask")
	)
	(pad "19" smd rect
		(at 1.7835 2.52)
		(size 2.72 1.27)
		(layers "F.Cu" "F.Mask")
	)
	(pad "19" smd rect
		(at 2.2535 3.4775)
		(size 0.25 0.645)
		(layers "F.Cu" "F.Mask")
	)
	(pad "19" smd rect
		(at 2.7535 3.4775)
		(size 0.25 0.645)
		(layers "F.Cu" "F.Mask")
	)
	(pad "19" smd rect
		(at 3.4685 2.25)
		(size 0.65 0.25)
		(layers "F.Cu" "F.Mask")
	)
	(pad "19" smd rect
		(at 3.4685 2.75)
		(size 0.65 0.25)
		(layers "F.Cu" "F.Mask")
	)
	(pad "20" smd rect
		(at -0.2465 3.425)
		(size 0.25 0.75)
		(layers "F.Cu" "F.Mask")
	)
	(pad "20" smd rect
		(at -0.0265 2.26)
		(size 0.25 1.98)
		(layers "F.Cu" "F.Mask")
	)
	(pad "20" smd rect
		(at 1.3835 0.84)
		(size 2.72 1.27)
		(layers "F.Cu" "F.Mask")
	)
	(pad "20" smd rect
		(at 3.2685 1.3)
		(size 1.05 0.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "21" smd rect
		(at 3.1435 0.5)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Mask")
	)
	(pad "21" smd rect
		(at 3.5185 0.25)
		(size 0.55 0.25)
		(layers "F.Cu" "F.Mask")
	)
	(pad "21" smd rect
		(at 3.5185 0.75)
		(size 0.55 0.25)
		(layers "F.Cu" "F.Mask")
	)
	(pad "22" smd rect
		(at 3.1435 -0.5)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Mask")
	)
	(pad "22" smd rect
		(at 3.5185 -0.75)
		(size 0.55 0.25)
		(layers "F.Cu" "F.Mask")
	)
	(pad "22" smd rect
		(at 3.5185 -0.25)
		(size 0.55 0.25)
		(layers "F.Cu" "F.Mask")
	)
	(pad "23" smd rect
		(at -0.2465 -3.425)
		(size 0.25 0.75)
		(layers "F.Cu" "F.Mask")
	)
	(pad "23" smd rect
		(at -0.0265 -2.26)
		(size 0.25 1.98)
		(layers "F.Cu" "F.Mask")
	)
	(pad "23" smd rect
		(at 1.3835 -0.84)
		(size 2.72 1.27)
		(layers "F.Cu" "F.Mask")
	)
	(pad "23" smd rect
		(at 3.2685 -1.3)
		(size 1.05 0.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "24" smd rect
		(at 0.7535 -3.4775)
		(size 0.25 0.645)
		(layers "F.Cu" "F.Mask")
	)
	(pad "24" smd rect
		(at 1.2535 -3.4775)
		(size 0.25 0.645)
		(layers "F.Cu" "F.Mask")
	)
	(pad "24" smd rect
		(at 1.7535 -3.4775)
		(size 0.25 0.645)
		(layers "F.Cu" "F.Mask")
	)
	(pad "24" smd rect
		(at 1.7865 -2.52)
		(size 2.72 1.27)
		(layers "F.Cu" "F.Mask")
	)
	(pad "24" smd rect
		(at 2.2535 -3.4775)
		(size 0.25 0.645)
		(layers "F.Cu" "F.Mask")
	)
	(pad "24" smd rect
		(at 2.7535 -3.4775)
		(size 0.25 0.645)
		(layers "F.Cu" "F.Mask")
	)
	(pad "24" smd rect
		(at 3.4715 -2.75)
		(size 0.65 0.25)
		(layers "F.Cu" "F.Mask")
	)
	(pad "24" smd rect
		(at 3.4715 -2.25)
		(size 0.65 0.25)
		(layers "F.Cu" "F.Mask")
	)
	(pad "26" smd rect
		(at -0.7465 -3.45)
		(size 0.25 0.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "27" smd rect
		(at -1.2465 -3.45)
		(size 0.25 0.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "29" smd rect
		(at -2.2465 -3.45)
		(size 0.25 0.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "30" smd rect
		(at -2.7465 -3.45)
		(size 0.25 0.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "31" smd rect
		(at -2.5465 -2.29 45)
		(size 0.283 0.282843)
		(layers "F.Cu" "F.Mask")
	)
	(pad "31" smd rect
		(at -1.7465 -3.145)
		(size 0.25 1.31)
		(layers "F.Cu" "F.Mask")
	)
	(pad "31" smd rect
		(at -1.7465 3.145)
		(size 0.25 1.31)
		(layers "F.Cu" "F.Mask")
	)
	(pad "31" smd rect
		(at -1.6665 0.1)
		(size 2.16 4.78)
		(layers "F.Cu" "F.Mask")
	)
	(pad "31" smd rect
		(at -1.5665 -2.39)
		(size 1.96 0.2)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Infineon_PQFN-44-31-5EP_7x7mm_P0.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
