(footprint "LQFN-16-1EP_3x3mm_P0.5mm_EP1.7x1.7mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "LQFN, 16 Pin (https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-lqfn/05081595_0_lqfn16.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "LQFN NoLead")
	(property "Reference" "REF**"
		(at 0 -2.83 0)
		(layer "F.SilkS")
	)
	(property "Value" "LQFN-16-1EP_3x3mm_P0.5mm_EP1.7x1.7mm"
		(at 0 2.83 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at 0 0)
		(size 1.37 1.37)
		(layers "F.Paste")
		(roundrect_rratio 0.182482)
	)
	(pad "1" smd roundrect
		(at -1.4625 -0.75)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -1.4625 -0.25)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -1.4625 0.25)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -1.4625 0.75)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -0.75 1.4625)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -0.25 1.4625)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at 0.25 1.4625)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 0.75 1.4625)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at 1.4625 0.75)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at 1.4625 0.25)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at 1.4625 -0.25)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at 1.4625 -0.75)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 0.75 -1.4625)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at 0.25 -1.4625)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at -0.25 -1.4625)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at -0.75 -1.4625)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd rect
		(at 0 0)
		(size 1.7 1.7)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/LQFN-16-1EP_3x3mm_P0.5mm_EP1.7x1.7mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
