(footprint "Linear_DE14MA"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "14-Lead Plastic DFN, 4mm x 3mm (http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-dfn/05081731_C_DE14MA.pdf)")
	(tags "DFN 0.5")
	(property "Reference" "REF**"
		(at 0 -3.05 0)
		(layer "F.SilkS")
	)
	(property "Value" "Linear_DE14MA"
		(at 0 3.05 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.4 -1.5)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.4 -1)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.4 -0.5)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd custom
		(at 0 -0.79)
		(size 1.65 1.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0.575 -0.64)
				(end 0.825 -0.64)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 0.575 0.64)
				(end 0.825 0.64)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.575 0.89) (xy -0.825 0.89) (xy -0.825 -0.64) (xy -0.575 -0.89) (xy 0.575 -0.89)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -0.78 0.89) (xy -0.88 0.915) (xy -1.75 0.915) (xy -1.75 0.665) (xy -0.78 0.665)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -0.825 0.665) (xy -1.075 0.665) (xy -1.025 0.66) (xy -0.977 0.645) (xy -0.935 0.622) (xy -0.897 0.591)
					(xy -0.866 0.552) (xy -0.844 0.511) (xy -0.83 0.464) (xy -0.825 0.415)
				)
				(width 0.001)
				(fill yes)
			)
		)
	)
	(pad "5" smd rect
		(at -1.4 0.5)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -1.4 1)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -1.4 1.5)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 1.4 1.5)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd custom
		(at 0 1.145)
		(size 1.15 1.07)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center -0.575 -0.285)
				(end -0.325 -0.285)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 0.575 -0.285)
				(end 0.825 -0.285)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -0.575 0.285)
				(end -0.325 0.285)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 0.575 0.285)
				(end 0.825 0.285)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.825 0.285) (xy -0.825 0.285) (xy -0.825 -0.285) (xy 0.825 -0.285)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.75 -0.02) (xy 0.825 -0.02) (xy 0.825 -0.27) (xy 1.75 -0.27)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "10" smd rect
		(at 1.4 0.5)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 1.4 0)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 1.4 -0.5)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 1.4 -1)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 1.4 -1.5)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Linear_DE14MA.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
