(footprint "MLF-8-1EP_3x3mm_P0.65mm_EP1.55x2.3mm_ThermalVias"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "8-Pin ePad 3mm x 3mm MLF - 3x3x0.85 mm Body (see Microchip datasheet http://ww1.microchip.com/downloads/en/DeviceDoc/mic5355_6.pdf)")
	(tags "DFN MLF 0.65")
	(property "Reference" "REF**"
		(at 0 -2.55 0)
		(layer "F.SilkS")
	)
	(property "Value" "MLF-8-1EP_3x3mm_P0.65mm_EP1.55x2.3mm_ThermalVias"
		(at 0 2.55 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at 0 -0.9)
		(size 1.5 0.4)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0 0)
		(size 1.5 0.65)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0 0.9)
		(size 1.5 0.4)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "1" smd roundrect
		(at -1.36 -0.975)
		(size 0.48 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -1.36 -0.325)
		(size 0.48 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -1.36 0.325)
		(size 0.48 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -1.36 0.975)
		(size 0.48 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 1.36 0.975)
		(size 0.48 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 1.36 0.325)
		(size 0.48 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at 1.36 -0.325)
		(size 0.48 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 1.36 -0.975)
		(size 0.48 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" thru_hole circle
		(at 0 -0.5)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" smd rect
		(at 0 0)
		(size 1.55 2.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "9" smd rect
		(at 0 0)
		(size 1.55 2.3)
		(layers "B.Cu")
	)
	(pad "9" thru_hole circle
		(at 0 0.5)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/MLF-8-1EP_3x3mm_P0.65mm_EP1.55x2.3mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
