(footprint "Maxim_FC2QFN-14_2.5x2.5mm_P0.5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "14-FC2QFN, 14/12 Pin, https://pdfserv.maximintegrated.com/land_patterns/90-100127.PDF")
	(tags "FC2QFN NoLead")
	(property "Reference" "REF**"
		(at 0 -2.55 0)
		(layer "F.SilkS")
	)
	(property "Value" "Maxim_FC2QFN-14_2.5x2.5mm_P0.5mm"
		(at 0 2.55 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -1.2375 -0.5)
		(size 0.675 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(chamfer_ratio 0.45)
		(chamfer top_right)
	)
	(pad "2" smd roundrect
		(at -1.2375 0)
		(size 0.675 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "3" smd roundrect
		(at -1.2375 0.5)
		(size 0.675 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "4" smd roundrect
		(at -0.75 1.2375)
		(size 0.3 0.675)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "5" smd roundrect
		(at -0.25 1.2375)
		(size 0.3 0.675)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "6" smd roundrect
		(at 0.5 1.2375)
		(size 0.8 0.675)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(chamfer_ratio 0.12)
		(chamfer top_right)
	)
	(pad "8" smd roundrect
		(at 1.2375 0.65)
		(size 0.675 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(chamfer_ratio 0.28)
		(chamfer bottom_left)
	)
	(pad "9" smd roundrect
		(at 1.2375 0)
		(size 0.675 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "10" smd roundrect
		(at 1.2375 -0.65)
		(size 0.675 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(chamfer_ratio 0.28)
		(chamfer top_left)
	)
	(pad "11" smd roundrect
		(at 0.5 -1.2375)
		(size 0.8 0.675)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(chamfer_ratio 0.12)
		(chamfer bottom_right)
	)
	(pad "13" smd roundrect
		(at -0.25 -1.2375)
		(size 0.3 0.675)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "14" smd roundrect
		(at -0.75 -1.2375)
		(size 0.3 0.675)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Maxim_FC2QFN-14_2.5x2.5mm_P0.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
