(footprint "Microchip_8E-16"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "16-Lead Quad Flat, No Lead Package (8E) - 4x4x0.9 mm Body [UQFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
	(tags "QFN Microchip 8E 16")
	(property "Reference" "REF**"
		(at 0 -3.1 0)
		(layer "F.SilkS")
	)
	(property "Value" "Microchip_8E-16"
		(at 0 3.1 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(solder_mask_margin 0.1)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.8125 -0.975)
		(size 0.725 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.8125 -0.325)
		(size 0.725 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.8125 0.325)
		(size 0.725 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.8125 0.975)
		(size 0.725 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -0.975 1.8125 90)
		(size 0.725 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -0.325 1.8125 90)
		(size 0.725 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 0.325 1.8125 90)
		(size 0.725 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 0.975 1.8125 90)
		(size 0.725 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 1.8125 0.975)
		(size 0.725 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 1.8125 0.325)
		(size 0.725 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 1.8125 -0.325)
		(size 0.725 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 1.8125 -0.975)
		(size 0.725 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 0.975 -1.8125 90)
		(size 0.725 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 0.325 -1.8125 90)
		(size 0.725 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -0.325 -1.8125 90)
		(size 0.725 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -0.975 -1.8125 90)
		(size 0.725 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -0.5375 -0.5375)
		(size 1.075 1.075)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio -0.2)
	)
	(pad "17" smd rect
		(at -0.5375 0.5375)
		(size 1.075 1.075)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio -0.2)
	)
	(pad "17" smd rect
		(at 0.5375 -0.5375)
		(size 1.075 1.075)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio -0.2)
	)
	(pad "17" smd rect
		(at 0.5375 0.5375)
		(size 1.075 1.075)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio -0.2)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-16-1EP_4x4mm_Pitch0.65mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
