(footprint "Microchip_DRQFN-44-1EP_5x5mm_P0.7mm_EP2.65x2.65mm_ThermalVias"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "QFN, 44 Pin, dual row (http://ww1.microchip.com/downloads/en/DeviceDoc/44L_VQFN_5x5mm_Dual_Row_%5BS3B%5D_C04-21399a.pdf)")
	(tags "QFN dual row")
	(property "Reference" "REF**"
		(at 0 -4 0)
		(layer "F.SilkS")
	)
	(property "Value" "Microchip_DRQFN-44-1EP_5x5mm_P0.7mm_EP2.65x2.65mm_ThermalVias"
		(at 0 4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.5 -0.5)
		(size 0.85 0.85)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -0.5 0.5)
		(size 0.85 0.85)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.5 -0.5)
		(size 0.85 0.85)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.5 0.5)
		(size 0.85 0.85)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "A1" smd oval
		(at -2.45 -1.75)
		(size 0.6 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd oval
		(at -2.45 -1.05)
		(size 0.6 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd oval
		(at -2.45 -0.35)
		(size 0.6 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A4" smd oval
		(at -2.45 0.35)
		(size 0.6 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A5" smd oval
		(at -2.45 1.05)
		(size 0.6 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A6" smd oval
		(at -2.45 1.75)
		(size 0.6 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A7" smd oval
		(at -1.75 2.45)
		(size 0.3 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A8" smd oval
		(at -1.05 2.45)
		(size 0.3 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A9" smd oval
		(at -0.35 2.45)
		(size 0.3 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A10" smd oval
		(at 0.35 2.45)
		(size 0.3 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A11" smd oval
		(at 1.05 2.45)
		(size 0.3 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A12" smd oval
		(at 1.75 2.45)
		(size 0.3 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A13" smd oval
		(at 2.45 1.75)
		(size 0.6 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A14" smd oval
		(at 2.45 1.05)
		(size 0.6 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A15" smd oval
		(at 2.45 0.35)
		(size 0.6 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A16" smd oval
		(at 2.45 -0.35)
		(size 0.6 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A17" smd oval
		(at 2.45 -1.05)
		(size 0.6 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A18" smd oval
		(at 2.45 -1.75)
		(size 0.6 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A19" smd oval
		(at 1.75 -2.45)
		(size 0.3 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A20" smd oval
		(at 1.05 -2.45)
		(size 0.3 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A21" smd oval
		(at 0.35 -2.45)
		(size 0.3 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A22" smd oval
		(at -0.35 -2.45)
		(size 0.3 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A23" smd oval
		(at -1.05 -2.45)
		(size 0.3 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A24" smd oval
		(at -1.75 -2.45)
		(size 0.3 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd oval
		(at -1.925 -1.4)
		(size 0.42 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B2" smd oval
		(at -1.925 -0.7)
		(size 0.42 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B3" smd oval
		(at -1.925 0)
		(size 0.42 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B4" smd oval
		(at -1.925 0.7)
		(size 0.42 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B5" smd oval
		(at -1.925 1.4)
		(size 0.42 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B6" smd oval
		(at -1.4 1.925)
		(size 0.3 0.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B7" smd oval
		(at -0.7 1.925)
		(size 0.3 0.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B8" smd oval
		(at 0 1.925)
		(size 0.3 0.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B9" smd oval
		(at 0.7 1.925)
		(size 0.3 0.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B10" smd oval
		(at 1.4 1.925)
		(size 0.3 0.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B11" smd oval
		(at 1.925 1.4)
		(size 0.42 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B12" smd oval
		(at 1.925 0.7)
		(size 0.42 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B13" smd oval
		(at 1.925 0)
		(size 0.42 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B14" smd oval
		(at 1.925 -0.7)
		(size 0.42 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B15" smd oval
		(at 1.925 -1.4)
		(size 0.42 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B16" smd oval
		(at 1.4 -1.925)
		(size 0.3 0.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B17" smd oval
		(at 0.7 -1.925)
		(size 0.3 0.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B18" smd oval
		(at 0 -1.925)
		(size 0.3 0.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B19" smd oval
		(at -0.7 -1.925)
		(size 0.3 0.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B20" smd oval
		(at -1.4 -1.925)
		(size 0.3 0.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "EP" thru_hole circle
		(at -1 -1)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "EP" thru_hole circle
		(at -1 0)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "EP" thru_hole circle
		(at -1 1)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "EP" thru_hole circle
		(at 0 -1)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "EP" thru_hole circle
		(at 0 0)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "EP" smd roundrect
		(at 0 0)
		(size 2.65 2.65)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.094)
	)
	(pad "EP" smd roundrect
		(at 0 0)
		(size 2.65 2.65)
		(layers "B.Cu")
		(roundrect_rratio 0.094)
	)
	(pad "EP" thru_hole circle
		(at 0 1)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "EP" thru_hole circle
		(at 1 -1)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "EP" thru_hole circle
		(at 1 0)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "EP" thru_hole circle
		(at 1 1)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Microchip_DRQFN-44-1EP_5x5mm_P0.7mm_EP2.65x2.65mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
