(footprint "Microchip_DRQFN-64-1EP_7x7mm_P0.65mm_EP4.1x4.1mm_ThermalVias"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "QFN, 64 Pin, dual row (http://ww1.microchip.com/downloads/en/DeviceDoc/64L_VQFN_7x7_Dual_Row_%5BSVB%5D_C04-21420a.pdf)")
	(tags "QFN dual row")
	(property "Reference" "REF**"
		(at 0 -5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Microchip_DRQFN-64-1EP_7x7mm_P0.65mm_EP4.1x4.1mm_ThermalVias"
		(at 0 5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -1.16 -1.16)
		(size 1 1)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -1.16 0)
		(size 1 1)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -1.16 1.16)
		(size 1 1)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0 -1.16)
		(size 1 1)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0 0)
		(size 1 1)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0 1.16)
		(size 1 1)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.16 -1.16)
		(size 1 1)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.16 0)
		(size 1 1)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.16 1.16)
		(size 1 1)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "A1" smd oval
		(at -3.45 -2.275)
		(size 0.7 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd oval
		(at -3.45 -1.625)
		(size 0.7 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd oval
		(at -3.45 -0.975)
		(size 0.7 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A4" smd oval
		(at -3.45 -0.325)
		(size 0.7 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A5" smd oval
		(at -3.45 0.325)
		(size 0.7 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A6" smd oval
		(at -3.45 0.975)
		(size 0.7 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A7" smd oval
		(at -3.45 1.625)
		(size 0.7 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A8" smd oval
		(at -3.45 2.275)
		(size 0.7 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A9" smd oval
		(at -2.6 3.45)
		(size 0.37 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A10" smd oval
		(at -1.95 3.45)
		(size 0.37 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A11" smd oval
		(at -1.3 3.45)
		(size 0.37 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A12" smd oval
		(at -0.65 3.45)
		(size 0.37 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A13" smd oval
		(at 0 3.45)
		(size 0.37 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A14" smd oval
		(at 0.65 3.45)
		(size 0.37 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A15" smd oval
		(at 1.3 3.45)
		(size 0.37 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A16" smd oval
		(at 1.95 3.45)
		(size 0.37 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A17" smd oval
		(at 2.6 3.45)
		(size 0.37 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A18" smd oval
		(at 3.45 2.275)
		(size 0.7 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A19" smd oval
		(at 3.45 1.625)
		(size 0.7 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A20" smd oval
		(at 3.45 0.975)
		(size 0.7 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A21" smd oval
		(at 3.45 0.325)
		(size 0.7 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A22" smd oval
		(at 3.45 -0.325)
		(size 0.7 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A23" smd oval
		(at 3.45 -0.975)
		(size 0.7 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A24" smd oval
		(at 3.45 -1.625)
		(size 0.7 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A25" smd oval
		(at 3.45 -2.275)
		(size 0.7 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A26" smd oval
		(at 2.6 -3.45)
		(size 0.37 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A27" smd oval
		(at 1.95 -3.45)
		(size 0.37 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A28" smd oval
		(at 1.3 -3.45)
		(size 0.37 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A29" smd oval
		(at 0.65 -3.45)
		(size 0.37 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A30" smd oval
		(at 0 -3.45)
		(size 0.37 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A31" smd oval
		(at -0.65 -3.45)
		(size 0.37 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A32" smd oval
		(at -1.3 -3.45)
		(size 0.37 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A33" smd oval
		(at -1.95 -3.45)
		(size 0.37 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A34" smd oval
		(at -2.6 -3.45)
		(size 0.37 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd oval
		(at -2.65 -1.95)
		(size 0.54 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B2" smd oval
		(at -2.65 -1.3)
		(size 0.54 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B3" smd oval
		(at -2.65 -0.65)
		(size 0.54 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B4" smd oval
		(at -2.65 0)
		(size 0.54 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B5" smd oval
		(at -2.65 0.65)
		(size 0.54 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B6" smd oval
		(at -2.65 1.3)
		(size 0.54 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B7" smd oval
		(at -2.65 1.95)
		(size 0.54 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B8" smd oval
		(at -2.275 2.65)
		(size 0.37 0.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B9" smd oval
		(at -1.625 2.65)
		(size 0.37 0.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B10" smd oval
		(at -0.975 2.65)
		(size 0.37 0.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B11" smd oval
		(at -0.325 2.65)
		(size 0.37 0.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B12" smd oval
		(at 0.325 2.65)
		(size 0.37 0.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B13" smd oval
		(at 0.975 2.65)
		(size 0.37 0.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B14" smd oval
		(at 1.625 2.65)
		(size 0.37 0.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B15" smd oval
		(at 2.275 2.65)
		(size 0.37 0.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B16" smd oval
		(at 2.65 1.95)
		(size 0.54 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B17" smd oval
		(at 2.65 1.3)
		(size 0.54 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B18" smd oval
		(at 2.65 0.65)
		(size 0.54 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B19" smd oval
		(at 2.65 0)
		(size 0.54 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B20" smd oval
		(at 2.65 -0.65)
		(size 0.54 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B21" smd oval
		(at 2.65 -1.3)
		(size 0.54 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B22" smd oval
		(at 2.65 -1.95)
		(size 0.54 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B23" smd oval
		(at 2.275 -2.65)
		(size 0.37 0.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B24" smd oval
		(at 1.625 -2.65)
		(size 0.37 0.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B25" smd oval
		(at 0.975 -2.65)
		(size 0.37 0.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B26" smd oval
		(at 0.325 -2.65)
		(size 0.37 0.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B27" smd oval
		(at -0.325 -2.65)
		(size 0.37 0.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B28" smd oval
		(at -0.975 -2.65)
		(size 0.37 0.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B29" smd oval
		(at -1.625 -2.65)
		(size 0.37 0.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B30" smd oval
		(at -2.275 -2.65)
		(size 0.37 0.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "EP" thru_hole circle
		(at -1.74 -1.74)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "EP" thru_hole circle
		(at -1.74 -0.58)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "EP" thru_hole circle
		(at -1.74 0.58)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "EP" thru_hole circle
		(at -1.74 1.74)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "EP" thru_hole circle
		(at -0.58 -1.74)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "EP" thru_hole circle
		(at -0.58 -0.58)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "EP" thru_hole circle
		(at -0.58 0.58)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "EP" thru_hole circle
		(at -0.58 1.74)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "EP" smd roundrect
		(at 0 0)
		(size 4.1 4.1)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.06)
	)
	(pad "EP" smd roundrect
		(at 0 0)
		(size 4.1 4.1)
		(layers "B.Cu")
		(roundrect_rratio 0.06)
	)
	(pad "EP" thru_hole circle
		(at 0.58 -1.74)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "EP" thru_hole circle
		(at 0.58 -0.58)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "EP" thru_hole circle
		(at 0.58 0.58)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "EP" thru_hole circle
		(at 0.58 1.74)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "EP" thru_hole circle
		(at 1.74 -1.74)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "EP" thru_hole circle
		(at 1.74 -0.58)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "EP" thru_hole circle
		(at 1.74 0.58)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "EP" thru_hole circle
		(at 1.74 1.74)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Microchip_DRQFN-64-1EP_7x7mm_P0.65mm_EP4.1x4.1mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
