(footprint "Microsemi_QFN-40-32-2EP_6x8mm_P0.5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "40-Lead (32-Lead Populated) Plastic Quad Flat, No Lead Package - 6x8x0.9mm Body (https://www.microsemi.com/document-portal/doc_download/131677-pd70224-data-sheet)")
	(tags "QFN 0.5")
	(property "Reference" "REF**"
		(at 0 -5.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "Microsemi_QFN-40-32-2EP_6x8mm_P0.5mm"
		(at 0 5.2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -1.04 -2.06)
		(size 1.68 1.68)
		(layers "F.Paste")
		(solder_paste_margin_ratio -0.2)
	)
	(pad "" smd rect
		(at -1.04 1.425)
		(size 1.68 2.95)
		(layers "F.Paste")
		(solder_paste_margin_ratio -0.2)
	)
	(pad "" smd rect
		(at 1.04 -2.06)
		(size 1.68 1.68)
		(layers "F.Paste")
		(solder_paste_margin_ratio -0.2)
	)
	(pad "" smd rect
		(at 1.04 1.425)
		(size 1.68 2.95)
		(layers "F.Paste")
		(solder_paste_margin_ratio -0.2)
	)
	(pad "1" smd rect
		(at -2.92 -2.75)
		(size 0.56 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1" smd circle
		(at -2.64 -2.75)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -2.92 -2.25)
		(size 0.56 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd circle
		(at -2.64 -2.25)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -2.92 -1.75)
		(size 0.56 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd circle
		(at -2.64 -1.75)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -2.92 -0.75)
		(size 0.56 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd circle
		(at -2.64 -0.75)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -2.92 -0.25)
		(size 0.56 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd circle
		(at -2.64 -0.25)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -2.92 0.25)
		(size 0.56 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd circle
		(at -2.64 0.25)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -2.92 0.75)
		(size 0.56 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd circle
		(at -2.64 0.75)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -2.92 1.75)
		(size 0.56 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd circle
		(at -2.64 1.75)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -2.92 2.25)
		(size 0.56 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd circle
		(at -2.64 2.25)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -2.92 2.75)
		(size 0.56 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd circle
		(at -2.64 2.75)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd circle
		(at -1.75 3.645)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -1.75 3.925)
		(size 0.28 0.56)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd circle
		(at -1.25 3.645)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -1.25 3.925)
		(size 0.28 0.56)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd circle
		(at -0.25 3.645)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -0.25 3.925)
		(size 0.28 0.56)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd circle
		(at 0.25 3.645)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 0.25 3.925)
		(size 0.28 0.56)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd circle
		(at 1.25 3.645)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 1.25 3.925)
		(size 0.28 0.56)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd circle
		(at 1.75 3.645)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 1.75 3.925)
		(size 0.28 0.56)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd circle
		(at 2.64 2.75)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at 2.92 2.75)
		(size 0.56 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd circle
		(at 2.64 2.25)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 2.92 2.25)
		(size 0.56 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd circle
		(at 2.64 1.75)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at 2.92 1.75)
		(size 0.56 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd circle
		(at 2.64 0.75)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 2.92 0.75)
		(size 0.56 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd circle
		(at 2.64 0.25)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at 2.92 0.25)
		(size 0.56 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd circle
		(at 2.64 -0.25)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 2.92 -0.25)
		(size 0.56 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd circle
		(at 2.64 -0.75)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at 2.92 -0.75)
		(size 0.56 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd circle
		(at 2.64 -1.75)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 2.92 -1.75)
		(size 0.56 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd circle
		(at 2.64 -2.25)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at 2.92 -2.25)
		(size 0.56 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd circle
		(at 2.64 -2.75)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 2.92 -2.75)
		(size 0.56 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at 1.75 -3.925)
		(size 0.28 0.56)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd circle
		(at 1.75 -3.645)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 1.25 -3.925)
		(size 0.28 0.56)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd circle
		(at 1.25 -3.645)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 0.25 -3.925)
		(size 0.28 0.56)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd circle
		(at 0.25 -3.645)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at -0.25 -3.925)
		(size 0.28 0.56)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd circle
		(at -0.25 -3.645)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at -1.25 -3.925)
		(size 0.28 0.56)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd circle
		(at -1.25 -3.645)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at -1.75 -3.925)
		(size 0.28 0.56)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd circle
		(at -1.75 -3.645)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" thru_hole circle
		(at -1.68 -2.62)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at -1.68 -1.5)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at -0.56 -2.62)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at -0.56 -1.5)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "33" smd rect
		(at 0 -2.06)
		(size 4.37 2.29)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin -0.155)
		(solder_paste_margin_ratio -0.2)
	)
	(pad "33" smd rect
		(at 0 -2.06)
		(size 4.37 2.29)
		(layers "B.Cu" "B.Mask")
		(solder_mask_margin -0.155)
		(solder_paste_margin_ratio -0.2)
	)
	(pad "33" thru_hole circle
		(at 0.56 -2.62)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at 0.56 -1.5)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at 1.68 -2.62)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at 1.68 -1.5)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "34" thru_hole circle
		(at -1.68 0.305)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "34" thru_hole circle
		(at -1.68 1.425)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "34" thru_hole circle
		(at -1.68 2.545)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "34" thru_hole circle
		(at -0.56 0.305)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "34" thru_hole circle
		(at -0.56 1.425)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "34" thru_hole circle
		(at -0.56 2.545)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "34" smd rect
		(at 0 1.425)
		(size 4.37 3.56)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin -0.155)
		(solder_paste_margin_ratio -0.2)
	)
	(pad "34" smd rect
		(at 0 1.425)
		(size 4.37 3.56)
		(layers "B.Cu" "B.Mask")
		(solder_mask_margin -0.155)
		(solder_paste_margin_ratio -0.2)
	)
	(pad "34" thru_hole circle
		(at 0.56 0.305)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "34" thru_hole circle
		(at 0.56 1.425)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "34" thru_hole circle
		(at 0.56 2.545)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "34" thru_hole circle
		(at 1.68 0.305)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "34" thru_hole circle
		(at 1.68 1.425)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "34" thru_hole circle
		(at 1.68 2.545)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Microsemi_QFN-40-32-2EP_6x8mm_P0.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
