(footprint "NXP_LQFN-48-1EP_7x7mm_P0.5mm_EP3.5x3.5mm_16xMask0.45x0.45_ThermalVias"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "LQFN, 48 Pin (https://www.nxp.com/docs/en/package-information/98ASA00694D.pdf)")
	(tags "NXP LQFN NoLead")
	(property "Reference" "REF**"
		(at 0 -4.82 0)
		(layer "F.SilkS")
	)
	(property "Value" "NXP_LQFN-48-1EP_7x7mm_P0.5mm_EP3.5x3.5mm_16xMask0.45x0.45_ThermalVias"
		(at 0 4.82 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -1.5 -1.5)
		(size 0.45 0.45)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at -1.5 -0.5)
		(size 0.45 0.45)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at -1.5 0.5)
		(size 0.45 0.45)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at -1.5 1.5)
		(size 0.45 0.45)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at -0.5 -1.5)
		(size 0.45 0.45)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at -0.5 -0.5)
		(size 0.45 0.45)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at -0.5 0.5)
		(size 0.45 0.45)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at -0.5 1.5)
		(size 0.45 0.45)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 0.5 -1.5)
		(size 0.45 0.45)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 0.5 -0.5)
		(size 0.45 0.45)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 0.5 0.5)
		(size 0.45 0.45)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 0.5 1.5)
		(size 0.45 0.45)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 1.5 -1.5)
		(size 0.45 0.45)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 1.5 -0.5)
		(size 0.45 0.45)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 1.5 0.5)
		(size 0.45 0.45)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 1.5 1.5)
		(size 0.45 0.45)
		(layers "F.Mask" "F.Paste")
	)
	(pad "1" smd roundrect
		(at -3.375 -2.75)
		(size 0.85 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -3.375 -2.25)
		(size 0.85 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -3.375 -1.75)
		(size 0.85 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -3.375 -1.25)
		(size 0.85 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -3.375 -0.75)
		(size 0.85 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -3.375 -0.25)
		(size 0.85 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -3.375 0.25)
		(size 0.85 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -3.375 0.75)
		(size 0.85 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -3.375 1.25)
		(size 0.85 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -3.375 1.75)
		(size 0.85 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at -3.375 2.25)
		(size 0.85 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at -3.375 2.75)
		(size 0.85 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at -2.75 3.375)
		(size 0.27 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at -2.25 3.375)
		(size 0.27 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at -1.75 3.375)
		(size 0.27 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at -1.25 3.375)
		(size 0.27 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at -0.75 3.375)
		(size 0.27 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at -0.25 3.375)
		(size 0.27 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at 0.25 3.375)
		(size 0.27 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at 0.75 3.375)
		(size 0.27 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at 1.25 3.375)
		(size 0.27 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at 1.75 3.375)
		(size 0.27 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at 2.25 3.375)
		(size 0.27 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at 2.75 3.375)
		(size 0.27 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd roundrect
		(at 3.375 2.75)
		(size 0.85 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "26" smd roundrect
		(at 3.375 2.25)
		(size 0.85 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "27" smd roundrect
		(at 3.375 1.75)
		(size 0.85 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd roundrect
		(at 3.375 1.25)
		(size 0.85 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "29" smd roundrect
		(at 3.375 0.75)
		(size 0.85 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "30" smd roundrect
		(at 3.375 0.25)
		(size 0.85 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "31" smd roundrect
		(at 3.375 -0.25)
		(size 0.85 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "32" smd roundrect
		(at 3.375 -0.75)
		(size 0.85 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "33" smd roundrect
		(at 3.375 -1.25)
		(size 0.85 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "34" smd roundrect
		(at 3.375 -1.75)
		(size 0.85 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "35" smd roundrect
		(at 3.375 -2.25)
		(size 0.85 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "36" smd roundrect
		(at 3.375 -2.75)
		(size 0.85 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "37" smd roundrect
		(at 2.75 -3.375)
		(size 0.27 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "38" smd roundrect
		(at 2.25 -3.375)
		(size 0.27 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "39" smd roundrect
		(at 1.75 -3.375)
		(size 0.27 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "40" smd roundrect
		(at 1.25 -3.375)
		(size 0.27 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "41" smd roundrect
		(at 0.75 -3.375)
		(size 0.27 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "42" smd roundrect
		(at 0.25 -3.375)
		(size 0.27 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "43" smd roundrect
		(at -0.25 -3.375)
		(size 0.27 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "44" smd roundrect
		(at -0.75 -3.375)
		(size 0.27 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "45" smd roundrect
		(at -1.25 -3.375)
		(size 0.27 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "46" smd roundrect
		(at -1.75 -3.375)
		(size 0.27 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "47" smd roundrect
		(at -2.25 -3.375)
		(size 0.27 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "48" smd roundrect
		(at -2.75 -3.375)
		(size 0.27 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "49" thru_hole circle
		(at -1 -1)
		(size 0.55 0.55)
		(drill 0.25)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "49" thru_hole circle
		(at -1 0)
		(size 0.55 0.55)
		(drill 0.25)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "49" thru_hole circle
		(at -1 1)
		(size 0.55 0.55)
		(drill 0.25)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "49" thru_hole circle
		(at 0 -1)
		(size 0.55 0.55)
		(drill 0.25)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "49" thru_hole circle
		(at 0 0)
		(size 0.55 0.55)
		(drill 0.25)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "49" smd roundrect
		(at 0 0)
		(size 2.55 2.55)
		(layers "B.Cu")
		(roundrect_rratio 0.115)
	)
	(pad "49" smd rect
		(at 0 0)
		(size 3.5 3.5)
		(layers "F.Cu")
	)
	(pad "49" thru_hole circle
		(at 0 1)
		(size 0.55 0.55)
		(drill 0.25)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "49" thru_hole circle
		(at 1 -1)
		(size 0.55 0.55)
		(drill 0.25)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "49" thru_hole circle
		(at 1 0)
		(size 0.55 0.55)
		(drill 0.25)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "49" thru_hole circle
		(at 1 1)
		(size 0.55 0.55)
		(drill 0.25)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/NXP_LQFN-48-1EP_7x7mm_P0.5mm_EP3.5x3.5mm_16xMask0.45x0.45.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
