(footprint "Nordic_AQFN-73-1EP_7x7mm_P0.5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "http://infocenter.nordicsemi.com/index.jsp?topic=%2Fcom.nordic.infocenter.nrf52%2Fdita%2Fnrf52%2Fchips%2Fnrf52840.html")
	(tags "AQFN 7mm ")
	(property "Reference" "REF**"
		(at 0 -4.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Nordic_AQFN-73-1EP_7x7mm_P0.5mm"
		(at 0.03 5.72 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -1.2125 -1.2125 180)
		(size 2 2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.2125 1.2125 180)
		(size 2 2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.2125 -1.2125 180)
		(size 2 2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.2125 1.2125 180)
		(size 2 2)
		(layers "F.Paste")
	)
	(pad "A8" smd circle
		(at -1.25 -3.25 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A10" smd circle
		(at -0.75 -3.25 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A12" smd circle
		(at -0.25 -3.25 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A14" smd circle
		(at 0.25 -3.25 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A16" smd circle
		(at 0.75 -3.25 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A18" smd circle
		(at 1.25 -3.25 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A20" smd circle
		(at 1.75 -3.25 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A22" smd circle
		(at 2.25 -3.25 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A23" smd circle
		(at 2.75 -3.25 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA24" smd circle
		(at 3.25 2.25 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB2" smd circle
		(at -2.75 2.5 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC5" smd circle
		(at -2 2.75 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC9" smd circle
		(at -1 2.75 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC11" smd circle
		(at -0.5 2.75 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC13" smd circle
		(at 0 2.75 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC15" smd circle
		(at 0.5 2.75 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC17" smd circle
		(at 1 2.75 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC19" smd circle
		(at 1.5 2.75 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC21" smd circle
		(at 2 2.75 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC24" smd circle
		(at 3.25 2.75 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD2" smd circle
		(at -2.75 3.25 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD4" smd circle
		(at -2.25 3.25 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD6" smd circle
		(at -1.75 3.25 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD8" smd circle
		(at -1.25 3.25 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD10" smd circle
		(at -0.75 3.25 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD12" smd circle
		(at -0.25 3.25 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD14" smd circle
		(at 0.25 3.25 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD16" smd circle
		(at 0.75 3.25 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD18" smd circle
		(at 1.25 3.25 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD20" smd circle
		(at 1.75 3.25 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD22" smd circle
		(at 2.25 3.25 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD23" smd circle
		(at 2.75 3.25 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd circle
		(at -3.25 -2.75 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B3" smd circle
		(at -2.5 -2.75 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B5" smd circle
		(at -2 -2.75 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B7" smd circle
		(at -1.5 -2.75 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B9" smd circle
		(at -1 -2.75 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B11" smd circle
		(at -0.5 -2.75 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B13" smd circle
		(at 0 -2.75 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B15" smd circle
		(at 0.5 -2.75 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B17" smd circle
		(at 1 -2.75 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B19" smd circle
		(at 1.5 -2.75 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B24" smd circle
		(at 3.25 -2.75 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C1" smd circle
		(at -3.25 -2.25 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D2" smd circle
		(at -2.75 -2 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D23" smd circle
		(at 2.75 -2 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E24" smd circle
		(at 3.25 -1.75 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "EP" smd rect
		(at 0 0 180)
		(size 4.85 4.85)
		(layers "F.Cu" "F.Mask")
	)
	(pad "F2" smd circle
		(at -2.75 -1.5 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F23" smd circle
		(at 2.75 -1.5 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G1" smd circle
		(at -3.25 -1.25 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H2" smd circle
		(at -2.75 -1 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H23" smd circle
		(at 2.75 -1 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J1" smd circle
		(at -3.25 -0.75 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J24" smd circle
		(at 3.25 -0.75 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K2" smd circle
		(at -2.75 -0.5 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L1" smd circle
		(at -3.25 -0.25 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L24" smd circle
		(at 3.25 -0.25 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M2" smd circle
		(at -2.75 0 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N1" smd circle
		(at -3.25 0.25 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N24" smd circle
		(at 3.25 0.25 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P2" smd circle
		(at -2.75 0.5 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P23" smd circle
		(at 2.75 0.5 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R1" smd circle
		(at -3.25 0.75 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R24" smd circle
		(at 3.25 0.75 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T2" smd circle
		(at -2.75 1 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T23" smd circle
		(at 2.75 1 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U1" smd circle
		(at -3.25 1.25 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U24" smd circle
		(at 3.25 1.25 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V23" smd circle
		(at 2.75 1.5 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W1" smd circle
		(at -3.25 1.75 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W24" smd circle
		(at 3.25 1.75 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y2" smd circle
		(at -2.75 2 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y23" smd circle
		(at 2.75 2 180)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Nordic_AQFN-73-1EP_7x7mm_P0.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
