(footprint "Nordic_AQFN-94-1EP_7x7mm_P0.4mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "aQFN, Nordic, nRF5340, https://infocenter.nordicsemi.com/pdf/nRF5340_PS_v1.2.pdf")
	(tags "aqfn qfn nordic nrf nrf5340 aqfn94")
	(property "Reference" "REF**"
		(at 0 -4.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Nordic_AQFN-94-1EP_7x7mm_P0.4mm"
		(at 0 5.8 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd circle
		(at -3.2 -3.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "" smd circle
		(at -3.2 3.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at -1.1 -1.2 180)
		(size 2.2 2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.1 1.225 180)
		(size 2.2 2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.5 -1.2 180)
		(size 2.2 2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.5 1.225 180)
		(size 2.2 2)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 3.2 -3.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "" smd circle
		(at 3.2 3.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A5" smd circle
		(at -2.2 -3.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A13" smd circle
		(at -0.6 -3.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A15" smd circle
		(at -0.2 -3.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A17" smd circle
		(at 0.2 -3.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A19" smd circle
		(at 0.6 -3.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A21" smd circle
		(at 1 -3.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A23" smd circle
		(at 1.4 -3.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A25" smd circle
		(at 1.8 -3.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A27" smd circle
		(at 2.2 -3.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA1" smd circle
		(at -3.2 1)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA31" smd circle
		(at 3.2 1)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB2" smd circle
		(at -2.8 1.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC1" smd circle
		(at -3.2 1.4)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC31" smd circle
		(at 3.2 1.4)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD2" smd circle
		(at -2.8 1.6)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE1" smd circle
		(at -3.2 1.8)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE31" smd circle
		(at 3.2 1.8)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF2" smd circle
		(at -2.8 2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AG1" smd circle
		(at -3.2 2.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AG31" smd circle
		(at 3.2 2.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AH2" smd circle
		(at -2.8 2.4)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AJ1" smd circle
		(at -3.2 2.6)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AJ31" smd circle
		(at 3.2 2.6)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AK2" smd circle
		(at -2.8 2.8)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AK4" smd circle
		(at -2.4 2.8)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AK6" smd circle
		(at -2 2.8)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AK8" smd circle
		(at -1.6 2.8)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AK10" smd circle
		(at -1.2 2.8)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AK12" smd circle
		(at -0.8 2.8)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AK14" smd circle
		(at -0.4 2.8)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AK16" smd circle
		(at 0 2.8)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AK18" smd circle
		(at 0.4 2.8)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AK20" smd circle
		(at 0.8 2.8)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AK22" smd circle
		(at 1.2 2.8)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AK24" smd circle
		(at 1.6 2.8)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AK26" smd circle
		(at 2 2.8)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AK28" smd circle
		(at 2.4 2.8)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AK30" smd circle
		(at 2.8 2.8)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AL3" smd circle
		(at -2.6 3.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AL5" smd circle
		(at -2.2 3.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AL7" smd circle
		(at -1.8 3.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AL9" smd circle
		(at -1.4 3.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AL11" smd circle
		(at -1 3.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AL13" smd circle
		(at -0.6 3.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AL15" smd circle
		(at -0.2 3.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AL17" smd circle
		(at 0.2 3.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AL19" smd circle
		(at 0.6 3.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AL21" smd circle
		(at 1 3.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AL23" smd circle
		(at 1.4 3.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AL25" smd circle
		(at 1.8 3.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AL27" smd circle
		(at 2.2 3.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AL29" smd circle
		(at 2.6 3.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B2" smd circle
		(at -2.8 -2.8)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B4" smd circle
		(at -2.4 -2.8)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B6" smd circle
		(at -2 -2.8)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B8" smd circle
		(at -1.6 -2.8)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B10" smd circle
		(at -1.2 -2.8)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B12" smd circle
		(at -0.8 -2.8)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B14" smd circle
		(at -0.4 -2.8)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B16" smd circle
		(at 0 -2.8)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B18" smd circle
		(at 0.4 -2.8)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B20" smd circle
		(at 0.8 -2.8)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B22" smd circle
		(at 1.2 -2.8)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B24" smd circle
		(at 1.6 -2.8)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B26" smd circle
		(at 2 -2.8)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B28" smd circle
		(at 2.4 -2.8)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B30" smd circle
		(at 2.8 -2.8)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C1" smd circle
		(at -3.2 -2.6)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C31" smd circle
		(at 3.2 -2.6)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D2" smd circle
		(at -2.8 -2.4)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E1" smd circle
		(at -3.2 -2.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E31" smd circle
		(at 3.2 -2.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "EP" smd rect
		(at 0.2 0 180)
		(size 5.4 5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "F2" smd circle
		(at -2.8 -2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G1" smd circle
		(at -3.2 -1.8)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G31" smd circle
		(at 3.2 -1.8)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H2" smd circle
		(at -2.8 -1.6)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J1" smd circle
		(at -3.2 -1.4)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J31" smd circle
		(at 3.2 -1.4)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K2" smd circle
		(at -2.8 -1.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L1" smd circle
		(at -3.2 -1)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L31" smd circle
		(at 3.2 -1)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M2" smd circle
		(at -2.8 -0.8)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N1" smd circle
		(at -3.2 -0.6)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N31" smd circle
		(at 3.2 -0.6)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P2" smd circle
		(at -2.8 -0.4)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R1" smd circle
		(at -3.2 -0.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R31" smd circle
		(at 3.2 -0.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T2" smd circle
		(at -2.8 0)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U1" smd circle
		(at -3.2 0.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U31" smd circle
		(at 3.2 0.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V2" smd circle
		(at -2.8 0.4)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W1" smd circle
		(at -3.2 0.6)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W31" smd circle
		(at 3.2 0.6)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y2" smd circle
		(at -2.8 0.8)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Nordic_AQFN-94-1EP_7x7mm_P0.4mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
