(footprint "OnSemi_SIP-38-6EP-9x7mm_P0.65mm_EP1.2x1.2mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "On Semiconductor, SIP-38, 9x7mm, (https://www.onsemi.com/pub/Collateral/AX-SIP-SFEU-D.PDF#page=19)")
	(tags "On Semiconductor SIP")
	(property "Reference" "REF**"
		(at -2.65 -4.4 180)
		(layer "F.SilkS")
	)
	(property "Value" "OnSemi_SIP-38-6EP-9x7mm_P0.65mm_EP1.2x1.2mm"
		(at 0 4.45 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -4.1 -2.275)
		(size 0.5 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd oval
		(at -4.1 -1.625)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd oval
		(at -4.1 -0.975)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd oval
		(at -4.1 -0.325)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd oval
		(at -4.1 0.325)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd oval
		(at -4.1 0.975)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd oval
		(at -4.1 1.625)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd oval
		(at -4.1 2.275)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd oval
		(at -3.25 3.1 90)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd oval
		(at -2.6 3.1 90)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd oval
		(at -1.95 3.1 90)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd oval
		(at -1.3 3.1 90)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd oval
		(at -0.65 3.1 90)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd oval
		(at 0 3.1 90)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd oval
		(at 0.65 3.1 90)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd oval
		(at 1.3 3.1 90)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd oval
		(at 1.95 3.1 90)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd oval
		(at 2.6 3.1 90)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd oval
		(at 3.25 3.1 90)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd oval
		(at 4.1 2.275)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd oval
		(at 4.1 1.625)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd oval
		(at 4.1 0.975)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd oval
		(at 4.1 0.325)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd oval
		(at 4.1 -0.325)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd oval
		(at 4.1 -0.975)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd oval
		(at 4.1 -1.625)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd oval
		(at 4.1 -2.275)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd oval
		(at 3.25 -3.1 90)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd oval
		(at 2.6 -3.1 90)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd oval
		(at 1.95 -3.1 90)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd oval
		(at 1.3 -3.1 90)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd oval
		(at 0.65 -3.1 90)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd oval
		(at 0 -3.1 90)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd oval
		(at -0.65 -3.1 90)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd oval
		(at -1.3 -3.1 90)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd oval
		(at -1.95 -3.1 90)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd oval
		(at -2.6 -3.1 90)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd oval
		(at -3.25 -3.1 90)
		(size 0.501 0.351)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at -2 -1)
		(size 1.2 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd rect
		(at -2 1)
		(size 1.2 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd rect
		(at 0 1)
		(size 1.2 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd rect
		(at 2 1)
		(size 1.2 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd rect
		(at 2 -1)
		(size 1.2 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd rect
		(at 0 -1)
		(size 1.2 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/OnSemi_SIP-38-6EP-9x7mm_P0.65mm_EP1.2x1.2mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
