(footprint "OnSemi_UDFN-8_1.2x1.8mm_P0.4mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "8-Lead Plastic Dual Flat, No Lead Package, 1.2x1.8x1.55 mm Body [UDFN] (See http://www.onsemi.com/pub/Collateral/NLSV2T244-D.PDF)")
	(tags "dfn udfn dual flat")
	(property "Reference" "REF**"
		(at 0 -2 0)
		(layer "F.SilkS")
	)
	(property "Value" "OnSemi_UDFN-8_1.2x1.8mm_P0.4mm"
		(at 0 1.8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0.05 0 90)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -0.42 -0.65)
		(size 0.66 0.32)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -0.42 -0.2)
		(size 0.66 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -0.42 0.2)
		(size 0.66 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -0.42 0.6)
		(size 0.66 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 0.42 0.6)
		(size 0.66 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 0.42 0.2)
		(size 0.66 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 0.42 -0.2)
		(size 0.66 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 0.42 -0.6)
		(size 0.66 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/OnSemi_UDFN-8_1.2x1.8mm_P0.4mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
