(footprint "OnSemi_VCT-28_3.5x3.5mm_P0.4mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "OnSemi  VCT, 28 Pin (http://www.onsemi.com/pub/Collateral/601AE.PDF), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "OnSemi VCT NoLead")
	(property "Reference" "REF**"
		(at 0 -3.05 0)
		(layer "F.SilkS")
	)
	(property "Value" "OnSemi_VCT-28_3.5x3.5mm_P0.4mm"
		(at 0 3.05 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd custom
		(at -1.7375 -1.2)
		(size 0.13636 0.13636)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.3125 -0.05) (xy 0.251789 -0.05) (xy 0.3125 0.010711) (xy 0.3125 0.05) (xy -0.3125 0.05)
				)
				(width 0.1)
				(fill yes)
			)
		)
	)
	(pad "2" smd roundrect
		(at -1.6875 -0.8)
		(size 0.825 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -1.6875 -0.4)
		(size 0.825 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -1.6875 0)
		(size 0.825 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -1.6875 0.4)
		(size 0.825 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -1.6875 0.8)
		(size 0.825 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd custom
		(at -1.7375 1.2)
		(size 0.13636 0.13636)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.3125 -0.05) (xy 0.3125 -0.05) (xy 0.3125 -0.010711) (xy 0.251789 0.05) (xy -0.3125 0.05)
				)
				(width 0.1)
				(fill yes)
			)
		)
	)
	(pad "8" smd custom
		(at -1.2 1.7375)
		(size 0.13636 0.13636)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.05 -0.251789) (xy 0.010711 -0.3125) (xy 0.05 -0.3125) (xy 0.05 0.3125) (xy -0.05 0.3125)
				)
				(width 0.1)
				(fill yes)
			)
		)
	)
	(pad "9" smd roundrect
		(at -0.8 1.6875)
		(size 0.2 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -0.4 1.6875)
		(size 0.2 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at 0 1.6875)
		(size 0.2 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at 0.4 1.6875)
		(size 0.2 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 0.8 1.6875)
		(size 0.2 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd custom
		(at 1.2 1.7375)
		(size 0.13636 0.13636)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.05 -0.3125) (xy -0.010711 -0.3125) (xy 0.05 -0.251789) (xy 0.05 0.3125) (xy -0.05 0.3125)
				)
				(width 0.1)
				(fill yes)
			)
		)
	)
	(pad "15" smd custom
		(at 1.7375 1.2)
		(size 0.13636 0.13636)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.3125 -0.05) (xy 0.3125 -0.05) (xy 0.3125 0.05) (xy -0.251789 0.05) (xy -0.3125 -0.010711)
				)
				(width 0.1)
				(fill yes)
			)
		)
	)
	(pad "16" smd roundrect
		(at 1.6875 0.8)
		(size 0.825 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at 1.6875 0.4)
		(size 0.825 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at 1.6875 0)
		(size 0.825 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at 1.6875 -0.4)
		(size 0.825 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at 1.6875 -0.8)
		(size 0.825 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd custom
		(at 1.7375 -1.2)
		(size 0.13636 0.13636)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.3125 0.010711) (xy -0.251789 -0.05) (xy 0.3125 -0.05) (xy 0.3125 0.05) (xy -0.3125 0.05)
				)
				(width 0.1)
				(fill yes)
			)
		)
	)
	(pad "22" smd custom
		(at 1.2 -1.7375)
		(size 0.13636 0.13636)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.05 -0.3125) (xy 0.05 -0.3125) (xy 0.05 0.251789) (xy -0.010711 0.3125) (xy -0.05 0.3125)
				)
				(width 0.1)
				(fill yes)
			)
		)
	)
	(pad "23" smd roundrect
		(at 0.8 -1.6875)
		(size 0.2 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at 0.4 -1.6875)
		(size 0.2 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd roundrect
		(at 0 -1.6875)
		(size 0.2 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "26" smd roundrect
		(at -0.4 -1.6875)
		(size 0.2 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "27" smd roundrect
		(at -0.8 -1.6875)
		(size 0.2 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd custom
		(at -1.2 -1.7375)
		(size 0.13636 0.13636)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.05 -0.3125) (xy 0.05 -0.3125) (xy 0.05 0.3125) (xy 0.010711 0.3125) (xy -0.05 0.251789)
				)
				(width 0.1)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/OnSemi_VCT-28_3.5x3.5mm_P0.4mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
