(footprint "OnSemi_XDFN4-1EP_1.0x1.0mm_EP0.52x0.52mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "XDFN4 footprint (as found on the https://www.onsemi.com/pub/Collateral/NCP115-D.PDF)")
	(tags "OnSemi XDFN4")
	(property "Reference" "REF**"
		(at 0.11 1.6 0)
		(layer "F.SilkS")
	)
	(property "Value" "OnSemi_XDFN4-1EP_1.0x1.0mm_EP0.52x0.52mm"
		(at 0.5 -1.74 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 1.3 0)
		(layer "F.Fab")
	)
	(pad "1" smd custom
		(at -0.485 -0.325 270)
		(size 0.26 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.13 -0.115) (xy -0.13 -0.115) (xy -0.13 -0.275) (xy -0.02 -0.275)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "2" smd custom
		(at -0.485 0.325 270)
		(size 0.26 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.13 -0.115) (xy -0.13 -0.115) (xy 0.02 -0.275) (xy 0.13 -0.275)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "3" smd custom
		(at 0.485 0.325 90)
		(size 0.26 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.13 -0.115) (xy -0.13 -0.115) (xy -0.13 -0.275) (xy -0.02 -0.275)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "4" smd custom
		(at 0.485 -0.325 90)
		(size 0.26 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.13 -0.115) (xy -0.13 -0.115) (xy 0.02 -0.275) (xy 0.13 -0.275)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "5" smd rect
		(at 0 0 135)
		(size 0.52 0.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/OnSemi_XDFN4-1EP_1.0x1.0mm_EP0.52x0.52mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
