(footprint "Panasonic_HQFN-16-1EP_4x4mm_P0.65mm_EP2.9x2.9mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Panasonic HQFN-16, 4x4x0.85mm (https://industrial.panasonic.com/content/data/SC/ds/ds7/c0/PKG_HQFN016-A-0404XZL_EN.pdf)")
	(tags "panasonic hqfn")
	(property "Reference" "REF**"
		(at 0 -3.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "Panasonic_HQFN-16-1EP_4x4mm_P0.65mm_EP2.9x2.9mm"
		(at 0 3.2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(solder_mask_margin 0.05)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -1.95 -0.975)
		(size 0.5 0.36)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.95 -0.325)
		(size 0.5 0.36)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.95 0.325)
		(size 0.5 0.36)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.95 0.975)
		(size 0.5 0.36)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.975 -1.95)
		(size 0.36 0.5)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.975 1.95)
		(size 0.36 0.5)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.725 -0.725)
		(size 1.05 1.05)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.725 0.725)
		(size 1.05 1.05)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.325 -1.95)
		(size 0.36 0.5)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.325 1.95)
		(size 0.36 0.5)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.325 -1.95)
		(size 0.36 0.5)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.325 1.95)
		(size 0.36 0.5)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.725 -0.725)
		(size 1.05 1.05)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.725 0.725)
		(size 1.05 1.05)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.975 -1.95)
		(size 0.36 0.5)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.975 1.95)
		(size 0.36 0.5)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.95 -0.975)
		(size 0.5 0.36)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.95 -0.325)
		(size 0.5 0.36)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.95 0.325)
		(size 0.5 0.36)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.95 0.975)
		(size 0.5 0.36)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -1.925 -0.975)
		(size 0.55 0.36)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" smd rect
		(at -1.925 -0.325)
		(size 0.55 0.36)
		(layers "F.Cu" "F.Mask")
	)
	(pad "3" smd rect
		(at -1.925 0.325)
		(size 0.55 0.36)
		(layers "F.Cu" "F.Mask")
	)
	(pad "4" smd rect
		(at -1.925 0.975)
		(size 0.55 0.36)
		(layers "F.Cu" "F.Mask")
	)
	(pad "5" smd rect
		(at -0.975 1.925)
		(size 0.36 0.55)
		(layers "F.Cu" "F.Mask")
	)
	(pad "6" smd rect
		(at -0.325 1.925)
		(size 0.36 0.55)
		(layers "F.Cu" "F.Mask")
	)
	(pad "7" smd rect
		(at 0.325 1.925)
		(size 0.36 0.55)
		(layers "F.Cu" "F.Mask")
	)
	(pad "8" smd rect
		(at 0.975 1.925)
		(size 0.36 0.55)
		(layers "F.Cu" "F.Mask")
	)
	(pad "9" smd rect
		(at 1.925 0.975)
		(size 0.55 0.36)
		(layers "F.Cu" "F.Mask")
	)
	(pad "10" smd rect
		(at 1.925 0.325)
		(size 0.55 0.36)
		(layers "F.Cu" "F.Mask")
	)
	(pad "11" smd rect
		(at 1.925 -0.325)
		(size 0.55 0.36)
		(layers "F.Cu" "F.Mask")
	)
	(pad "12" smd rect
		(at 1.925 -0.975)
		(size 0.55 0.36)
		(layers "F.Cu" "F.Mask")
	)
	(pad "13" smd rect
		(at 0.975 -1.925)
		(size 0.36 0.55)
		(layers "F.Cu" "F.Mask")
	)
	(pad "14" smd rect
		(at 0.325 -1.925)
		(size 0.36 0.55)
		(layers "F.Cu" "F.Mask")
	)
	(pad "15" smd rect
		(at -0.325 -1.925)
		(size 0.36 0.55)
		(layers "F.Cu" "F.Mask")
	)
	(pad "16" smd rect
		(at -0.975 -1.925)
		(size 0.36 0.55)
		(layers "F.Cu" "F.Mask")
	)
	(pad "17" smd rect
		(at 0 0)
		(size 2.9 2.9)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Panasonic_HQFN-16-1EP_4x4mm_P0.65mm_EP2.9x2.9mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
