(footprint "Panasonic_HSON-8_8x8mm_P2.00mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Panasonic HSON-8, 8x8x1.25mm (https://industrial.panasonic.com/content/data/SC/ds/ds7/c0/PKG_HSON008-A-0808XXI_EN.pdf)")
	(tags "panasonic hson")
	(property "Reference" "REF**"
		(at 0 -5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Panasonic_HSON-8_8x8mm_P2.00mm"
		(at 0 5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(solder_mask_margin 0.05)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -4 -3)
		(size 1 1.3)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -4 -1)
		(size 1 1.3)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -4 1)
		(size 1 1.3)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -4 3)
		(size 1 1.3)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.15 -3)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.15 -1.5)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.15 0)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.15 1.5)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.15 3)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.65 -3)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.65 -1.5)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.65 0)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.65 1.5)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.65 3)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 4 -3)
		(size 1 1.3)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 4 -1)
		(size 1 1.3)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 4 1)
		(size 1 1.3)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 4 3)
		(size 1 1.3)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -3.975 -3)
		(size 1.05 1.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" smd rect
		(at -3.975 -1)
		(size 1.05 1.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "3" smd rect
		(at -3.975 1)
		(size 1.05 1.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "4" smd rect
		(at -3.975 3)
		(size 1.05 1.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "5" smd rect
		(at 3.975 3)
		(size 1.05 1.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "6" smd rect
		(at 3.975 1)
		(size 1.05 1.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "7" smd rect
		(at 3.975 -1)
		(size 1.05 1.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "8" smd rect
		(at 3.975 -3)
		(size 1.05 1.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "9" smd rect
		(at 0.9 0)
		(size 3.2 6.94)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Panasonic_HSON-8_8x8mm_P2.00mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
