(footprint "QFN-20-1EP_4x5mm_P0.5mm_EP2.65x3.65mm_ThermalVias"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "QFN, 20 Pin (http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-qfn/QFN_20_05-08-1711.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "QFN NoLead")
	(property "Reference" "REF**"
		(at 0 -3.83 0)
		(layer "F.SilkS")
	)
	(property "Value" "QFN-20-1EP_4x5mm_P0.5mm_EP2.65x3.65mm_ThermalVias"
		(at 0 3.83 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at -0.5375 -1.05)
		(size 0.787174 0.787174)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.376193 -0.240646)
					(xy -0.280817 -0.336022)
					(xy 0.280817 -0.336022)
					(xy 0.376193 -0.240646)
					(xy 0.376193 0.240646)
					(xy 0.280817 0.336022)
					(xy -0.280817 0.336022)
					(xy -0.376193 0.240646)
				)
				(width 0.230259)
			)
		)
	)
	(pad "" smd custom
		(at -0.5375 0)
		(size 0.787174 0.787174)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.376193 -0.240646)
					(xy -0.280817 -0.336022)
					(xy 0.280817 -0.336022)
					(xy 0.376193 -0.240646)
					(xy 0.376193 0.240646)
					(xy 0.280817 0.336022)
					(xy -0.280817 0.336022)
					(xy -0.376193 0.240646)
				)
				(width 0.230259)
			)
		)
	)
	(pad "" smd custom
		(at -0.5375 1.05)
		(size 0.787174 0.787174)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.376193 -0.240646)
					(xy -0.280817 -0.336022)
					(xy 0.280817 -0.336022)
					(xy 0.376193 -0.240646)
					(xy 0.376193 0.240646)
					(xy 0.280817 0.336022)
					(xy -0.280817 0.336022)
					(xy -0.376193 0.240646)
				)
				(width 0.230259)
			)
		)
	)
	(pad "" smd custom
		(at 0.5375 -1.05)
		(size 0.787174 0.787174)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.376193 -0.240646)
					(xy -0.280817 -0.336022)
					(xy 0.280817 -0.336022)
					(xy 0.376193 -0.240646)
					(xy 0.376193 0.240646)
					(xy 0.280817 0.336022)
					(xy -0.280817 0.336022)
					(xy -0.376193 0.240646)
				)
				(width 0.230259)
			)
		)
	)
	(pad "" smd custom
		(at 0.5375 0)
		(size 0.787174 0.787174)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.376193 -0.240646)
					(xy -0.280817 -0.336022)
					(xy 0.280817 -0.336022)
					(xy 0.376193 -0.240646)
					(xy 0.376193 0.240646)
					(xy 0.280817 0.336022)
					(xy -0.280817 0.336022)
					(xy -0.376193 0.240646)
				)
				(width 0.230259)
			)
		)
	)
	(pad "" smd custom
		(at 0.5375 1.05)
		(size 0.787174 0.787174)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.376193 -0.240646)
					(xy -0.280817 -0.336022)
					(xy 0.280817 -0.336022)
					(xy 0.376193 -0.240646)
					(xy 0.376193 0.240646)
					(xy 0.280817 0.336022)
					(xy -0.280817 0.336022)
					(xy -0.376193 0.240646)
				)
				(width 0.230259)
			)
		)
	)
	(pad "1" smd roundrect
		(at -1.95 -1.25)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -1.95 -0.75)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -1.95 -0.25)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -1.95 0.25)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -1.95 0.75)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -1.95 1.25)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -0.75 2.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -0.25 2.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at 0.25 2.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at 0.75 2.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at 1.95 1.25)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at 1.95 0.75)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 1.95 0.25)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at 1.95 -0.25)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at 1.95 -0.75)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at 1.95 -1.25)
		(size 0.85 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at 0.75 -2.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at 0.25 -2.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at -0.25 -2.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at -0.75 -2.45)
		(size 0.25 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "21" thru_hole circle
		(at -1.075 -1.575)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at -1.075 -0.525)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at -1.075 0.525)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at -1.075 1.575)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 0 -1.575)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 0 -0.525)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" smd rect
		(at 0 0)
		(size 2.65 3.65)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(pad "21" smd rect
		(at 0 0)
		(size 2.65 3.65)
		(property pad_prop_heatsink)
		(layers "B.Cu")
		(zone_connect 2)
	)
	(pad "21" thru_hole circle
		(at 0 0.525)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 0 1.575)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 1.075 -1.575)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 1.075 -0.525)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 1.075 0.525)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 1.075 1.575)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-20-1EP_4x5mm_P0.5mm_EP2.65x3.65mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
