(footprint "QFN-24-1EP_3x3mm_P0.4mm_EP1.75x1.6mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "QFN, 24 Pin (https://www.invensense.com/wp-content/uploads/2015/02/PS-MPU-9250A-01-v1.1.pdf#page=39), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "QFN NoLead")
	(property "Reference" "REF**"
		(at 0 -2.83 0)
		(layer "F.SilkS")
	)
	(property "Value" "QFN-24-1EP_3x3mm_P0.4mm_EP1.75x1.6mm"
		(at 0 2.83 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.44 -0.4)
		(size 0.71 0.64)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -0.44 0.4)
		(size 0.71 0.64)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.44 -0.4)
		(size 0.71 0.64)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.44 0.4)
		(size 0.71 0.64)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "1" smd custom
		(at -1.5 -1)
		(size 0.115147 0.115147)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.335 -0.06)
					(xy 0.238431 -0.06)
					(xy 0.335 0.036569)
					(xy 0.335 0.06)
					(xy -0.335 0.06)
				)
				(width 0.08)
			)
		)
	)
	(pad "2" smd roundrect
		(at -1.5 -0.6)
		(size 0.75 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -1.5 -0.2)
		(size 0.75 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -1.5 0.2)
		(size 0.75 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -1.5 0.6)
		(size 0.75 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd custom
		(at -1.5 1)
		(size 0.115147 0.115147)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.335 -0.06)
					(xy 0.335 -0.06)
					(xy 0.335 -0.036569)
					(xy 0.238431 0.06)
					(xy -0.335 0.06)
				)
				(width 0.08)
			)
		)
	)
	(pad "7" smd custom
		(at -1 1.5)
		(size 0.115147 0.115147)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.06 -0.238431)
					(xy 0.036569 -0.335)
					(xy 0.06 -0.335)
					(xy 0.06 0.335)
					(xy -0.06 0.335)
				)
				(width 0.08)
			)
		)
	)
	(pad "8" smd roundrect
		(at -0.6 1.5)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -0.2 1.5)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at 0.2 1.5)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at 0.6 1.5)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd custom
		(at 1 1.5)
		(size 0.115147 0.115147)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.06 -0.335)
					(xy -0.036569 -0.335)
					(xy 0.06 -0.238431)
					(xy 0.06 0.335)
					(xy -0.06 0.335)
				)
				(width 0.08)
			)
		)
	)
	(pad "13" smd custom
		(at 1.5 1)
		(size 0.115147 0.115147)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.335 -0.06)
					(xy 0.335 -0.06)
					(xy 0.335 0.06)
					(xy -0.238431 0.06)
					(xy -0.335 -0.036569)
				)
				(width 0.08)
			)
		)
	)
	(pad "14" smd roundrect
		(at 1.5 0.6)
		(size 0.75 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at 1.5 0.2)
		(size 0.75 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at 1.5 -0.2)
		(size 0.75 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at 1.5 -0.6)
		(size 0.75 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd custom
		(at 1.5 -1)
		(size 0.115147 0.115147)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.335 0.036569)
					(xy -0.238431 -0.06)
					(xy 0.335 -0.06)
					(xy 0.335 0.06)
					(xy -0.335 0.06)
				)
				(width 0.08)
			)
		)
	)
	(pad "19" smd custom
		(at 1 -1.5)
		(size 0.115147 0.115147)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.06 -0.335)
					(xy 0.06 -0.335)
					(xy 0.06 0.238431)
					(xy -0.036569 0.335)
					(xy -0.06 0.335)
				)
				(width 0.08)
			)
		)
	)
	(pad "20" smd roundrect
		(at 0.6 -1.5)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at 0.2 -1.5)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at -0.2 -1.5)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at -0.6 -1.5)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd custom
		(at -1 -1.5)
		(size 0.115147 0.115147)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.06 -0.335)
					(xy 0.06 -0.335)
					(xy 0.06 0.335)
					(xy 0.036569 0.335)
					(xy -0.06 0.238431)
				)
				(width 0.08)
			)
		)
	)
	(pad "25" smd rect
		(at 0 0)
		(size 1.75 1.6)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-24-1EP_3x3mm_P0.4mm_EP1.75x1.6mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
