(footprint "QFN-24-1EP_5x5mm_P0.65mm_EP3.6x3.6mm_ThermalVias"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "QFN, 24 Pin (https://www.nxp.com/docs/en/package-information/98ASA00734D.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "QFN NoLead")
	(property "Reference" "REF**"
		(at 0 -3.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "QFN-24-1EP_5x5mm_P0.65mm_EP3.6x3.6mm_ThermalVias"
		(at 0 3.8 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at -1.5375 -1.5375)
		(size 0.295204 0.295204)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.105817 -0.105817)
					(xy 0.105817 -0.105817)
					(xy 0.105817 -0.013308)
					(xy -0.013308 0.105817)
					(xy -0.105817 0.105817)
				)
				(width 0.211634)
			)
		)
	)
	(pad "" smd custom
		(at -1.5375 -0.85)
		(size 0.317469 0.317469)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.105835 -0.236847)
					(xy 0.018188 -0.236847)
					(xy 0.105835 -0.149199)
					(xy 0.105835 0.149199)
					(xy 0.018188 0.236847)
					(xy -0.105835 0.236847)
				)
				(width 0.211599)
			)
		)
	)
	(pad "" smd custom
		(at -1.5375 0)
		(size 0.317469 0.317469)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.105835 -0.236847)
					(xy 0.018188 -0.236847)
					(xy 0.105835 -0.149199)
					(xy 0.105835 0.149199)
					(xy 0.018188 0.236847)
					(xy -0.105835 0.236847)
				)
				(width 0.211599)
			)
		)
	)
	(pad "" smd custom
		(at -1.5375 0.85)
		(size 0.317469 0.317469)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.105835 -0.236847)
					(xy 0.018188 -0.236847)
					(xy 0.105835 -0.149199)
					(xy 0.105835 0.149199)
					(xy 0.018188 0.236847)
					(xy -0.105835 0.236847)
				)
				(width 0.211599)
			)
		)
	)
	(pad "" smd custom
		(at -1.5375 1.5375)
		(size 0.295204 0.295204)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.105817 -0.105817)
					(xy -0.013308 -0.105817)
					(xy 0.105817 0.013308)
					(xy 0.105817 0.105817)
					(xy -0.105817 0.105817)
				)
				(width 0.211634)
			)
		)
	)
	(pad "" smd custom
		(at -0.85 -1.5375)
		(size 0.317469 0.317469)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.236847 -0.105835)
					(xy 0.236847 -0.105835)
					(xy 0.236847 0.018188)
					(xy 0.149199 0.105835)
					(xy -0.149199 0.105835)
					(xy -0.236847 0.018188)
				)
				(width 0.211599)
			)
		)
	)
	(pad "" smd custom
		(at -0.85 -0.85)
		(size 0.601758 0.601758)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.259112 -0.189911)
					(xy -0.189911 -0.259112)
					(xy 0.189911 -0.259112)
					(xy 0.259112 -0.189911)
					(xy 0.259112 0.189911)
					(xy 0.189911 0.259112)
					(xy -0.189911 0.259112)
					(xy -0.259112 0.189911)
				)
				(width 0.167068)
			)
		)
	)
	(pad "" smd custom
		(at -0.85 0)
		(size 0.601758 0.601758)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.259112 -0.189911)
					(xy -0.189911 -0.259112)
					(xy 0.189911 -0.259112)
					(xy 0.259112 -0.189911)
					(xy 0.259112 0.189911)
					(xy 0.189911 0.259112)
					(xy -0.189911 0.259112)
					(xy -0.259112 0.189911)
				)
				(width 0.167068)
			)
		)
	)
	(pad "" smd custom
		(at -0.85 0.85)
		(size 0.601758 0.601758)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.259112 -0.189911)
					(xy -0.189911 -0.259112)
					(xy 0.189911 -0.259112)
					(xy 0.259112 -0.189911)
					(xy 0.259112 0.189911)
					(xy 0.189911 0.259112)
					(xy -0.189911 0.259112)
					(xy -0.259112 0.189911)
				)
				(width 0.167068)
			)
		)
	)
	(pad "" smd custom
		(at -0.85 1.5375)
		(size 0.317469 0.317469)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.236847 -0.018188)
					(xy -0.149199 -0.105835)
					(xy 0.149199 -0.105835)
					(xy 0.236847 -0.018188)
					(xy 0.236847 0.105835)
					(xy -0.236847 0.105835)
				)
				(width 0.211599)
			)
		)
	)
	(pad "" smd custom
		(at 0 -1.5375)
		(size 0.317469 0.317469)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.236847 -0.105835)
					(xy 0.236847 -0.105835)
					(xy 0.236847 0.018188)
					(xy 0.149199 0.105835)
					(xy -0.149199 0.105835)
					(xy -0.236847 0.018188)
				)
				(width 0.211599)
			)
		)
	)
	(pad "" smd custom
		(at 0 -0.85)
		(size 0.601758 0.601758)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.259112 -0.189911)
					(xy -0.189911 -0.259112)
					(xy 0.189911 -0.259112)
					(xy 0.259112 -0.189911)
					(xy 0.259112 0.189911)
					(xy 0.189911 0.259112)
					(xy -0.189911 0.259112)
					(xy -0.259112 0.189911)
				)
				(width 0.167068)
			)
		)
	)
	(pad "" smd custom
		(at 0 0)
		(size 0.601758 0.601758)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.259112 -0.189911)
					(xy -0.189911 -0.259112)
					(xy 0.189911 -0.259112)
					(xy 0.259112 -0.189911)
					(xy 0.259112 0.189911)
					(xy 0.189911 0.259112)
					(xy -0.189911 0.259112)
					(xy -0.259112 0.189911)
				)
				(width 0.167068)
			)
		)
	)
	(pad "" smd custom
		(at 0 0.85)
		(size 0.601758 0.601758)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.259112 -0.189911)
					(xy -0.189911 -0.259112)
					(xy 0.189911 -0.259112)
					(xy 0.259112 -0.189911)
					(xy 0.259112 0.189911)
					(xy 0.189911 0.259112)
					(xy -0.189911 0.259112)
					(xy -0.259112 0.189911)
				)
				(width 0.167068)
			)
		)
	)
	(pad "" smd custom
		(at 0 1.5375)
		(size 0.317469 0.317469)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.236847 -0.018188)
					(xy -0.149199 -0.105835)
					(xy 0.149199 -0.105835)
					(xy 0.236847 -0.018188)
					(xy 0.236847 0.105835)
					(xy -0.236847 0.105835)
				)
				(width 0.211599)
			)
		)
	)
	(pad "" smd custom
		(at 0.85 -1.5375)
		(size 0.317469 0.317469)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.236847 -0.105835)
					(xy 0.236847 -0.105835)
					(xy 0.236847 0.018188)
					(xy 0.149199 0.105835)
					(xy -0.149199 0.105835)
					(xy -0.236847 0.018188)
				)
				(width 0.211599)
			)
		)
	)
	(pad "" smd custom
		(at 0.85 -0.85)
		(size 0.601758 0.601758)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.259112 -0.189911)
					(xy -0.189911 -0.259112)
					(xy 0.189911 -0.259112)
					(xy 0.259112 -0.189911)
					(xy 0.259112 0.189911)
					(xy 0.189911 0.259112)
					(xy -0.189911 0.259112)
					(xy -0.259112 0.189911)
				)
				(width 0.167068)
			)
		)
	)
	(pad "" smd custom
		(at 0.85 0)
		(size 0.601758 0.601758)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.259112 -0.189911)
					(xy -0.189911 -0.259112)
					(xy 0.189911 -0.259112)
					(xy 0.259112 -0.189911)
					(xy 0.259112 0.189911)
					(xy 0.189911 0.259112)
					(xy -0.189911 0.259112)
					(xy -0.259112 0.189911)
				)
				(width 0.167068)
			)
		)
	)
	(pad "" smd custom
		(at 0.85 0.85)
		(size 0.601758 0.601758)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.259112 -0.189911)
					(xy -0.189911 -0.259112)
					(xy 0.189911 -0.259112)
					(xy 0.259112 -0.189911)
					(xy 0.259112 0.189911)
					(xy 0.189911 0.259112)
					(xy -0.189911 0.259112)
					(xy -0.259112 0.189911)
				)
				(width 0.167068)
			)
		)
	)
	(pad "" smd custom
		(at 0.85 1.5375)
		(size 0.317469 0.317469)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.236847 -0.018188)
					(xy -0.149199 -0.105835)
					(xy 0.149199 -0.105835)
					(xy 0.236847 -0.018188)
					(xy 0.236847 0.105835)
					(xy -0.236847 0.105835)
				)
				(width 0.211599)
			)
		)
	)
	(pad "" smd custom
		(at 1.5375 -1.5375)
		(size 0.295204 0.295204)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.105817 -0.105817)
					(xy 0.105817 -0.105817)
					(xy 0.105817 0.105817)
					(xy 0.013308 0.105817)
					(xy -0.105817 -0.013308)
				)
				(width 0.211634)
			)
		)
	)
	(pad "" smd custom
		(at 1.5375 -0.85)
		(size 0.317469 0.317469)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.105835 -0.149199)
					(xy -0.018188 -0.236847)
					(xy 0.105835 -0.236847)
					(xy 0.105835 0.236847)
					(xy -0.018188 0.236847)
					(xy -0.105835 0.149199)
				)
				(width 0.211599)
			)
		)
	)
	(pad "" smd custom
		(at 1.5375 0)
		(size 0.317469 0.317469)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.105835 -0.149199)
					(xy -0.018188 -0.236847)
					(xy 0.105835 -0.236847)
					(xy 0.105835 0.236847)
					(xy -0.018188 0.236847)
					(xy -0.105835 0.149199)
				)
				(width 0.211599)
			)
		)
	)
	(pad "" smd custom
		(at 1.5375 0.85)
		(size 0.317469 0.317469)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.105835 -0.149199)
					(xy -0.018188 -0.236847)
					(xy 0.105835 -0.236847)
					(xy 0.105835 0.236847)
					(xy -0.018188 0.236847)
					(xy -0.105835 0.149199)
				)
				(width 0.211599)
			)
		)
	)
	(pad "" smd custom
		(at 1.5375 1.5375)
		(size 0.295204 0.295204)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.105817 0.013308)
					(xy 0.013308 -0.105817)
					(xy 0.105817 -0.105817)
					(xy 0.105817 0.105817)
					(xy -0.105817 0.105817)
				)
				(width 0.211634)
			)
		)
	)
	(pad "1" smd roundrect
		(at -2.4375 -1.625)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -2.4375 -0.975)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -2.4375 -0.325)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -2.4375 0.325)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -2.4375 0.975)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -2.4375 1.625)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -1.625 2.4375)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -0.975 2.4375)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -0.325 2.4375)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at 0.325 2.4375)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at 0.975 2.4375)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at 1.625 2.4375)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 2.4375 1.625)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at 2.4375 0.975)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at 2.4375 0.325)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at 2.4375 -0.325)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at 2.4375 -0.975)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at 2.4375 -1.625)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at 1.625 -2.4375)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at 0.975 -2.4375)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at 0.325 -2.4375)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at -0.325 -2.4375)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at -0.975 -2.4375)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at -1.625 -2.4375)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "25" thru_hole circle
		(at -1.275 -1.275)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole circle
		(at -1.275 -0.425)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole circle
		(at -1.275 0.425)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole circle
		(at -1.275 1.275)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole circle
		(at -0.425 -1.275)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole circle
		(at -0.425 -0.425)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole circle
		(at -0.425 0.425)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole circle
		(at -0.425 1.275)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "25" smd rect
		(at 0 0)
		(size 3.05 3.05)
		(property pad_prop_heatsink)
		(layers "B.Cu")
		(zone_connect 2)
	)
	(pad "25" smd rect
		(at 0 0)
		(size 3.6 3.6)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(pad "25" thru_hole circle
		(at 0.425 -1.275)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole circle
		(at 0.425 -0.425)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole circle
		(at 0.425 0.425)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole circle
		(at 0.425 1.275)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole circle
		(at 1.275 -1.275)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole circle
		(at 1.275 -0.425)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole circle
		(at 1.275 0.425)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole circle
		(at 1.275 1.275)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-24-1EP_5x5mm_P0.65mm_EP3.6x3.6mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
